{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","","","30","34"]
["","","Kúrenie","Super nízke","m³/min","","","32","34"]
["Akustický výkon","Vykurovanie","","","dBA","","62","","","62"]
["","Chladenie","","","dBA","","60","","","60"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","cfm","","","1059","1200"]
["","","Kúrenie","Super nízke","cfm","","","1130","1200"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","550","550","550","550","550","550"]
["","","","Šírka","mm","765","765","765","765","765","765"]
["","","","Hĺbka","mm","285","285","285","285","285","285"]
["Hmotnosť","Jednotka","","","kg","36","36","36","41","41","41"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot./min.","500","500","760","890","500","500"]
["","","Kúrenie","Super nízke","ot./min.","320","320","820","890","500","500"]
["Kompresor","Type","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","","46.0","-10","-10","46.0"]
["","","","Max.","°CDB","","-10","46","46","-10"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","","-15","-15","-15","-15.0"]
["","","","Max.","° CWB","","18.0","18","18","18.0"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46","46","","","48","48"]
["","","","Men.","dBA","","","48","46"]
["","Kúrenie","","Vysoké","dBA","48","48","","","50","50"]
["","","","Men.","dBA","","","50","48"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Náplň","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Náplň","","","tCO2Eq","0.59","0.6","0.6","0.8","0.78","0.78"]
["","GWP","","","","675.0","675","675","675","675","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20","20 (1)","20","20","20 (1)","20"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 20m)","0,02 (pre potrubie s dĺžkou presahujúcou 20m)","002 (pre potrubie s dĺžkou presahujúcou 20m)","0,02 (pre potrubie s dĺžkou presahujúcou 20m)","0,02 (pre potrubie s dĺžkou presahujúcou 20m)","0,02 (pre potrubie s dĺžkou presahujúcou 20m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15.0","15","15","15","15","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","30","30","30","30","30","30"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Napätie","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Poznámky","","","","","(1) - Pre jednu miestnosť","","(1) - Obsahuje fluórované skleníkové plyny","","","(1) - Pre jednu miestnosť"]
["","","","","","","(1) - Pre jednu miestnosť","","","(1) - Pre jednu miestnosť"]
["","","","","","","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese","","","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch","","","(3) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","","","(4) - Obsahuje fluórované skleníkové plyny","","","(4) - Obsahuje fluórované skleníkové plyny"]
["Kompresor","Typ","","","","","","Hermeticky utesnený kolísavý kompresor"]
["Štandardné príslušenstvo","Reducer assembly","","","","","","","1","1","1"]