{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","734","734"]
["","","","Šírka","mm","974","974"]
["","","","Hĺbka","mm","401","401"]
["Hmotnosť","Jednotka","","","kg","57","57"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot/min","420","420"]
["","","Kúrenie","Super nízke","ot/min","420","420"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","46","46"]
["","Kúrenie","","Men.","dBA","47","47"]
["Chladivo","Typ","","","","R-32","R-32"]
["","Náplň","","","kg","1.8","1.8"]
["","Náplň","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","25","25 (1)"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 30m)","0,02 (pre potrubie s dĺžkou presahujúcou 30m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","50","50 (2)"]
["Štandardné príslušenstvo","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napájanie","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]
["Poznámky","","","","","(1) - Pre jednu miestnosť","(1) - Pre jednu miestnosť"]
["","","","","","(2) - Na kombináciu s CVXM-A, FVXM-A – maximálna dĺžka potrubia je 30 m.","(2) - Na kombináciu s CVXM-A, FVXM-A – maximálna dĺžka potrubia je 30 m."]