{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-G"]
[]
[]
[]
[]
["","","","","","3MXS68G2V1B"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","735"]
["","","","Šírka","mm","936"]
["","","","Hĺbka","mm","300"]
["Hmotnosť","Jednotka","","","kg","58"]
["Kompresor","Type","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15"]
["","","","Max.","°CWB","15.5"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","48"]
["","Kúrenie","","Men.","dBA","49"]
["Chladivo","Typ","","","","R-410A"]
["","Náplň","","","kg","2.59"]
["","Náplň","","","tCO2Eq","5.4"]
["","GWP","","","","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","25"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 30m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","50"]
["Štandardné príslušenstvo","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Air direction adjustment plate","","","","Air direction adjustment plate"]
["Napájanie","Fáza","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50"]
["","Napätie","","","V","230"]