{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B","4MXS80E3V3B2","4MXS80E7V3B"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","770","770"]
["","","","Šírka","mm","900","900"]
["","","","Hĺbka","mm","320","320"]
["Hmotnosť","Jednotka","","","kg","72","72"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","18","18"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","48","48"]
["","Kúrenie","","Men.","dBA","49","49"]
["Chladiace médium","Typ","","","","R-410A","R-410A"]
["","Náplň","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Pripojenia potrubia","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 30m)","0,02 (pre potrubie s dĺžkou presahujúcou 30m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15","15"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","70","70"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","1"]
["","Vypúšťacia skrutka","","","","1","1"]
["","Zostava redaktora","","","","1","1"]
["Power supply","Fáza","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","230","230"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota: 27 °CDB, 19,0 °CWB; vonkajšej teplote: 35 °CDB, ekvivalentná dĺžka potrubia: 7,5m","(1) - Chladenie: vnútorná teplota: 27 °CDB, 19,0 °CWB; vonkajšej teplote: 35 °CDB, ekvivalentná dĺžka potrubia: 7,5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5m","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5m"]
["","","","","","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","","770"]
["","","","Šírka","mm","","","900"]
["","","","Hĺbka","mm","","","320"]
["Hmotnosť","Jednotka","","","kg","","","72"]
["Kompresor","Typ","","","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","","","-15"]
["","","","Max.","°CWB","","","15.5"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","","","48"]
["","Kúrenie","","Men.","dBA","","","49"]
["Chladivo","Typ","","","","","","R-410A"]
["","Náplň","","","kg","","","2.99"]
["","Náplň","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","","","25"]
["","Dodatočná náplň chladiva","","","kg/m","","","0,02 (pre potrubie s dĺžkou presahujúcou 30m)"]
["","Úroveň hladiny","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","","","70"]
["Štandardné príslušenstvo","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Napájanie","Fáza","","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","","50"]
["","Napätie","","","V","","","230"]