{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":8,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-F"]
[]
[]
[]
[]
["","","","","","4MXS68F3V1B2","4MXS68F3V1B","4MXS68F2V1B"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","49","49"]
["","Chladenie","","Men.","dBA","48","48"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","1"]
["","Vypúšťacia skrutka","","","","1","1"]
["","Zostava redaktora","","","","1","1"]
["Chladiace médium","Charge","","","TCO2Eq","5.4","5.4"]
["","GWP","","","","2,087.5","2,087.5"]
["","Náplň","","","kg","2.6","2.6"]
["","Typ","","","","R-410A","R-410A"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Max.","°CDB","46"]
["","","","Min.","°CDB","-10"]
["","Kúrenie","Okolitá teplota","Max.","° CWB","18"]
["","","","Min.","° CWB","-15"]
["Pripojenia potrubia","Úroveň hladiny","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 30m)"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","60"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","936","936"]
["","","","Hĺbka","mm","300","300"]
["","","","Výška","mm","735","735"]
["Hmotnosť","Jednotka","","","kg","58","58"]
["Power supply","Fáza","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","230","230"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27 °CDB, 19,0 °CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 5m","(1) - Chladenie: vnútorná teplota 27 °CDB, 19,0 °CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 5m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m"]
["","","","","","(3) - Obsahuje fluórované skleníkové plyny","(3) - Obsahuje fluórované skleníkové plyny"]
["Pripojenia potrubia","Úroveň hladiny","IU - IU","Max.","m","","7.5"]
["","","IU - OU","Max.","m","","15"]
["","Dodatočná náplň chladiva","","","kg/m","","0,02 (pre potrubie s dĺžkou presahujúcou 30m)"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","","60"]
["Kompresor","Typ","","","","","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","","735"]
["","","","Šírka","mm","","","936"]
["","","","Hĺbka","mm","","","300"]
["Hmotnosť","Jednotka","","","kg","","","58"]
["Kompresor","Typ","","","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","","","-15"]
["","","","Max.","° CWB","","","15.5"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","","","48"]
["","Kúrenie","","Men.","dBA","","","49"]
["Chladivo","Typ","","","","","","R-410A"]
["","Náplň","","","kg","","","2.6"]
["","Náplň","","","tCO2Eq","","","5.4"]
["","GWP","","","","","","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","","","25"]
["","Dodatočná náplň chladiva","","","kg/m","","","0,02 (pre potrubie s dĺžkou presahujúcou 30m)"]
["","Úroveň hladiny","IU - OU","Max.","m","","","15"]
["","","IU - IU","Max.","m","","","7.5"]
["","Celková dĺžka potrubia","Systém","Skutočná","m","","","60"]
["Štandardné príslušenstvo","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Napájanie","Fáza","","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","","50"]
["","Napätie","","","V","","","230"]