{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Chladiaci výkon","Men.","","kW","9.5","12.1 (1)"]
["Chladenie","SEER","","","4.65","4.68"]
["","Ročná spotreba energie","","kWh/a","716","1,550"]
["","Výkon","P návrh","kW","9.50","12.1"]
["","Trieda energetickej účinnosti","","","B"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Trieda energetickej účinnosti","","","A"]
["","Ročná spotreba energie","","kWh/a","2,498","3,340"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Smernica o energetickom označovaní","Chladenie","","D"]
["","","Vykurovanie","","B"]
["Vykurovací výkon","Men.","","kW","10.8","13.5 (2)"]
["Poznámky","","","","(1) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m"]
["","","","","(2) - Ročná spotreba energie je podľa Smernice o energetickom označení 2002/31/ES","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]
["","","","","(3) - Hodnoty SEER a SCOP sú podľa normy EN 14825","(3) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","","(4) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]