{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Štandardné príslušenstvo","Návod na montáž","","","","Návod na montáž"]
["","Návod na prevádzku","","","","Návod na prevádzku"]
["","Skrutka + podložka","","","","Skrutka + podložka"]
["","Bezdrôtové diaľkové ovládanie","","","","Bezdrôtové diaľkové ovládanie"]
["","Zaisťovacia mriežka krytu","","","","Zaisťovacia mriežka krytu"]
["","Batéria","","","","Batéria"]
["Pripojenia potrubí","Liquid","","OD","mm","9.52"]
["","Plyn","","OD","mm","15.88"]
["","Drain","","","","19.05"]
["Vstup napájania","Chladenie","","Men.","kW","0.128"]
["","Kúrenie","","Men.","kW","0.128"]
["Úroveň akustického výkonu","Chladenie","","","dBA","64"]
["","Vykurovanie","","","dBA","64"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","600"]
["","","","Hĺbka","mm","1,007"]
["","","","Výška","mm","285"]
["Opláštenie","Material","","","","Pozinkovaná oceľ"]
["Hmotnosť","Jednotka","","","kg","35"]
["Ventilátor","Externý statický tlak","","Vysoké","Pa","90"]
["","","","Nom. ot.","Pa","77"]
["","","","Nízka","Pa","64"]
["Power supply","Fáza","","","","1~"]
["","Frekvencia","","","Hz","50"]
["","Názov","","","","V1"]
["","Napätie","","","V","220-240"]
["Vstup napájania","Kúrenie","","Men.","kW","","0.109"]
["","Chladenie","","Men.","kW","","0.109"]
["Ventilátor","Externý statický tlak","","Vysoký","Pa","","70","150","150"]
["","","","Nízky","Pa","","45","111","92"]
["Opláštenie","Materiál","","","","","Pozinkovaná oceľ"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","378","378","378"]
["","","","Šírka","mm","","541","1300","1500"]
["","","","Hĺbka","mm","","1045","541","541"]
["Hmotnosť","Jednotka","","","kg","","44","50","56"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","22.7","40.5","48.7"]
["","","","Men.","m³/min","","20.5","37","44"]
["","","","Nízka","m³/min","","18.3","34.8","37.9"]
["","","Kúrenie","Vysoké","m³/min","","22.7","40.5","48.7"]
["","","","Men.","m³/min","","20.5","37.4","43.9"]
["","","","Nízka","m³/min","","18.3","34.8","37.9"]
["","Externý statický tlak","","Nom. ot.","Pa","","57","128","122"]
["Akustický výkon","Chladenie","","","dBA","","60","72","73"]
["","Vykurovanie","","","dBA","","60","72","73"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","41","53","55"]
["","","","Men.","dBA","","38"]
["","","","Nízka","dBA","","36","50","50"]
["","Kúrenie","","Vysoké","dBA","","41","53","55"]
["","","","Men.","dBA","","38"]
["","","","Nízka","dBA","","36","50","50"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","9.52","9.52","9.52"]
["","Plyn","","OD","mm","","15.88","15.9","15.9"]
["","Odvod kondenzátu","","","","","19.05"]
["Štandardné príslušenstvo","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Napájanie","Fáza","","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","50"]
["","Napätie","","","V","","220-240"]
["Chladiaci výkon","Celkový výkon","","Men.","kW","","","12.10","13.00"]
["Vykurovací výkon","Celkový výkon","","Nom. ot.","kW","","","13.5","15.5"]
["Opláštenie","Farba","","","","","","Pozinkovaný oceľový plech/nenatretý","Pozinkovaný oceľový plech/nenatretý"]
["Ventilátor","Prietok vzduchu","Chladenie","Stredný","m³/min","","","37","44"]
["","","Vykurovanie","Stredný","m³/min","","","37.4","43.9"]
["Hladina akustického tlaku","Chladenie","","Stredný","dBA","","","52","53"]
["","Vykurovanie","","Stredný","dBA","","","52","53"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","","","ARCWLA","ARCWLA"]