{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Hladina akust. tlaku","Kúrenie","","Vysoké","dBA","","44","","47"]
["","","","Men.","dBA","","41","","44"]
["","","","Tichá prevádzka","dBA","","36","","41"]
["","","","Nízka","dBA","","38","","43"]
["","Chladenie","","Tichá prevádzka","dBA","","36","","41"]
["","","","Nízka","dBA","","38","","43"]
["","","","Vysoké","dBA","","44","","47"]
["","","","Men.","dBA","","41","","44"]
["Štandardné príslušenstvo","Návod na montáž","","","","","Návod na montáž","","Návod na montáž"]
["","Návod na prevádzku","","","","","Návod na prevádzku","","Návod na prevádzku"]
["","Skrutky","","","","","Skrutky","","Skrutky"]
["","Podložka","","","","","Podložka","","Podložka"]
["","Bezdrôtové diaľkové ovládanie","","","","","Bezdrôtové diaľkové ovládanie","","Bezdrôtové diaľkové ovládanie"]
["","Zaisťovacia mriežka krytu","","","","","Zaisťovacia mriežka krytu","","Zaisťovacia mriežka krytu"]
["","Batéria","","","","","Batéria","","Batéria"]
["Riadiace systémy","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","9.52","","9.52"]
["","Plyn","","OD","mm","","15.88","","15.88"]
["","Vypúšťanie","","","","","19.05","","19.05"]
["Vstup napájania","Chladenie","","Men.","kW","","0.094","","0.137"]
["","Kúrenie","","Men.","kW","","0.094","","0.137"]
["Úroveň akustického výkonu","Chladenie","","","dBA","","56","","60"]
["","Vykurovanie","","","dBA","","56","","60"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","820","","820"]
["","","","Hĺbka","mm","","820","","820"]
["","","","Výška","mm","","300","","300"]
["Kryt","Materiál","","","","","Pozinkovaná oceľ","","Pozinkovaná oceľ"]
["Hmotnosť","Jednotka","","","kg","","39","","39"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","","29.2","","34.0"]
["","","","Nízka","m³/min","","21.0","","26.3"]
["","","","Men.","m³/min","","24.4","","29.2"]
["","","Chladenie","Nízka","m³/min","","21.0","","26.3"]
["","","","Men.","m³/min","","24.4","","29.2"]
["","","","Vysoké","m³/min","","29.2","","34.0"]
["","","","Tichá prevádzka","m³/min","","17.6","","22.1"]
["","","Chladenie","Tichá prevádzka","m³/min","","17.6","","22.1"]
["Dekoračný panel","Hmotnosť","","","kg","","4","","4"]
["","Vonkajšie rozmery","","Výška","mm","","82","","82"]
["","","","Hĺbka","mm","","990","","990"]
["","","","Šírka","mm","","990","","990"]
["","Farba","","","","","Biela","","Biela"]
["Power supply","Fáza","","","","","1~","","1~"]
["","Názov","","","","","V1","","V1"]
["","Frekvencia","","","Hz","","50","","50"]
["","Napätie","","","V","","220-240","","220-240"]
["Ventilátor","Prietok vzduchu","Kúrenie","Tichá prevádzka","m³/min","15","","22.1"]
["Vstup napájania","Kúrenie","","Men.","kW","0.067","","0.137"]
["","Chladenie","","Men.","kW","0.067","","0.137"]
["Ventilátor","Prietok vzduchu","Chladenie","Tichá prevádzka","m³/min","15","","22.1"]
["Opláštenie","Materiál","","","","Pozinkovaná oceľ","","Pozinkovaná oceľ"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","265","","300"]
["","","","Šírka","mm","820","","820"]
["","","","Hĺbka","mm","820","","820"]
["Hmotnosť","Jednotka","","","kg","31","","39"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","24.4","","34"]
["","","","Men.","m³/min","20.5","","29.2"]
["","","","Nízka","m³/min","17.6","","26.3"]
["","","Kúrenie","Vysoké","m³/min","24.4","","34"]
["","","","Men.","m³/min","20.5","","29.2"]
["","","","Nízka","m³/min","17.6","","26.3"]
["Akustický výkon","Chladenie","","","dBA","54","","60"]
["","Vykurovanie","","","dBA","54","","60"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","41","","47"]
["","","","Men.","dBA","38","","44"]
["","","","Nízka","dBA","35","","43"]
["","","","Tichá prevádzka","dBA","32","","41"]
["","Kúrenie","","Vysoké","dBA","41","","47"]
["","","","Men.","dBA","38","","44"]
["","","","Nízka","dBA","35","","43"]
["","","","Tichá prevádzka","dBA","32","","41"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52","","9.52"]
["","Plyn","","OD","mm","15.88","","15.88"]
["","Odvod kondenzátu","","","","19.05","","19.05"]
["Dekoračný panel","Vonkajšie rozmery","","Výška","mm","82","","82"]
["","","","Šírka","mm","990","","990"]
["","","","Hĺbka","mm","990","","990"]
["","Hmotnosť","","","kg","4","","4"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","ARCWLA","","ARCWLA"]
["","Káblový diaľkový ovládač","","","","ARCWB","","ARCWB"]
["Štandardné príslušenstvo","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Napájanie","Fáza","","","","1~","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","","50"]
["","Napätie","","","V","220-240","","220-240"]