{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / ARXM-A9"]
[]
[]
[]
[]
["","","","","ADEA35A2VEB / ARXM35A5V1B9","ADEA50A2VEB / ARXM50A5V1B9"]
["Chladiaci výkon","Men.","","kW","3.4","5"]
["Vykurovací výkon","Men.","","kW","4","5.5"]
["Nominálna účinnosť","EER","","","3.76","3.27"]
["","COP","","","3.97","3.74"]
["","Ročná spotreba energie","","kWh","452","765"]
["","Smernica o energetickom označovaní","Chladenie","","A","A"]
["","","Vykurovanie","","A","A"]
["Chladenie","Trieda energetickej účinnosti","","","A+","A+"]
["","Výkon","P návrh","kW","3.4","5"]
["","SEER","","","5.9","5.65"]
["","Ročná spotreba energie","","kWh/rok","202","310"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A+","A+"]
["","Výkon","P návrh","kW","2.9","4.4"]
["","SCOP/A","","","4.07","4"]
["","Pdh Vykurovací výkon pri -10°","","kW","2.32","3.73"]
["","Ročná spotreba energie","","kWh/rok","997","1538"]
["Poznámky","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(3) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(4) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]