{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZAS-MY"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZAS100MUY","ADEA125A2VEB / AZAS125MUY"]
["Chladiaci výkon","Men.","","kW","9.5","12.1 (1)"]
["Vykurovací výkon","Men.","","kW","10.8 (2)","13.5 (2)"]
["Chladenie","Trieda energetickej účinnosti","","","A"]
["","Výkon","P návrh","kW","9.5","12.1"]
["","SEER","","","5.55","5.11"]
["","Ročná spotreba energie","","kWh/a","600","1421"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A"]
["","Výkon","P návrh","kW","6","6"]
["","SCOP/A","","","3.81","3.5"]
["","Ročná spotreba energie","","kWh/a","2205","2400"]
["Poznámky","","","","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]