{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Chladiaci výkon","Men.","","kW","9.50","12.10"]
["Chladenie","SEER","","","5.10","4.83"]
["","Ročná spotreba energie","","kWh/rok","652","1,504"]
["","Výkon","P návrh","kW","9.50","12.10"]
["","Trieda energetickej účinnosti","","","A"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Trieda energetickej účinnosti","","","A"]
["","Ročná spotreba energie","","kWh/rok","2,793","3,167"]
["Nominálna účinnosť","EER","","","","2.27"]
["Vykurovací výkon","Men.","","kW","10.80","13.50"]
["Poznámky","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","(3) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m","(3) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m"]
["","","","","(4) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m","(4) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]