{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C / ARXS-L3"]
[]
[]
[]
[]
["","","","ADEQ35C2VEB / ARXS35L3V1B"]
["Chladiaci výkon","Men.","kW","3.40 (1)"]
["Vykurovací výkon","Men.","kW","4.00 (1)"]
["Poznámky","","","(1) - Nominálna účinnosť: chladenie pri 35°/27° nomin. záťaž, vykurovanie pri 7°/20° nomin. záťaž"]
["","","","(2) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["","","","(3) - PED: montáž = kategória l: vylúčená z rozsahu PED kvôli článku 1, položka 3.6 Smernice 97/23/ES"]
["","","","(4) - Min. hodnota Ssc (= Skratový výkon): Zariadenie vyhovujúce norme EN 61000-3-2"]
["","","","(5) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","(6) - Obsahuje fluórované skleníkové plyny"]