{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":11,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARX-K"]
[]
[]
[]
[]
["","","","","","ARX20K2V1B","ARX20K5V1B9","ARX25K2V1B","ARX25K5V1B9","ARX35K2V1B","ARX35K5V1B9"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","550","550","550","550","550","550"]
["","","","Šírka","mm","658","658","658","658","658","658"]
["","","","Hĺbka","mm","275","275","275","275","275","275"]
["Hmotnosť","Jednotka","","","kg","28","26","28","26","28","28"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)"]
["","","","Max.","°CDB","46","46","46","46","46","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46","46","46","46","48","48"]
["","Kúrenie","","Vysoké","dBA","47","47","47","47","48","48"]
["Chladivo","Typ","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Náplň","","","kg","0.74","0.74","0.74","0.74","1.0","1.0"]
["","Náplň","","","tCO2Eq","1.5","1.5","1.5","1.5","2.1","2.1"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","15","15","15","15","15","15"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","12","12","12","12","12","12"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Poznámky","","","","","(1) - Prevádzkový rozsah v kombinácii s ATX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s ATX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s ATX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s ATX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s ATX-J3: min. 10°CDB ~ max. 46°CDB","(1) - Prevádzkový rozsah v kombinácii s ATX-J3: min. 10°CDB ~ max. 46°CDB"]
["Štandardné príslušenstvo","LOT10 Energy Label","","","","","LOT10 Energy Label","","LOT10 Energy Label","","LOT10 Energy Label"]