{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M"]
[]
[]
[]
[]
["","","","","","ARXM50MV1B","ARXM25M2V1B (Archived)","ARXM35M2V1B (Archived)"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","735","550","550"]
["","","","Šírka","mm","825","765","765"]
["","","","Hĺbka","mm","300","285","285"]
["Hmotnosť","Jednotka","","","kg","44","32","32"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","48","46","49"]
["","","","Nízka","dBA","44"]
["","Kúrenie","","Vysoké","dBA","49","47","49"]
["","","","Nízka","dBA","45"]
["Chladivo","Typ","","","","R-32","R-32","R-32"]
["","Náplň","","","kg","1.4","0.76","0.76"]
["","Náplň","","","tCO2Eq","0.9","0.5","0.5"]
["","GWP","","","","675","675","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","30","15","15"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","20","12","12"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1"]
["Napájanie","Fáza","","","","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240"]