{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","","49.0"]
["","Chladenie","","Men.","dBA","","49.0"]
["Štandardné príslušenstvo","Vypúšťacia skrutka","","","","","1"]
["","Návod na montáž","","","","","1"]
["","Štítok s náplňou chladiva","","","","","1"]
["","Viacjazyčné štítky o fluórovaných skleníkových plynoch","","","","","1"]
["","Všeobecné bezpečnostné opatrenia","","","","","1"]
["Chladivo","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Charge","","","kg","","0.76"]
["","Typ","","","","","R-32"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Max.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Pripojenia potrubia","Úroveň hladiny","IU - OU","Max.","m","","15"]
["","Dodatočná náplň chladiva","","","kg/m","","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["Kompresor","Typ","","","","","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","840"]
["","","","Hĺbka","mm","","350"]
["","","","Výška","mm","","552"]
["Hmotnosť","Jednotka","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Napätie","","","V","","220-240"]
["Poznámky","","","","","(1) - Možné len v kombinácii s ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Obsahuje fluórované skleníkové plyny"]
["","","","","","(2) - Možné len v kombinácii s ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch"]
["","","","","","","(4) - Možné len v kombinácii s ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Možné len v kombinácii s ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","552"]
["","","","Šírka","mm","840"]
["","","","Hĺbka","mm","350"]
["Hmotnosť","Jednotka","","","kg","32"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","-10"]
["","","","Max.","°CDB","50 (4), 46 (5)"]
["Hladina akustického tlaku","Chladenie","","Men.","dBA","46.0"]
["","Kúrenie","","Men.","dBA","47.0"]
["Chladivo","Náplň","","","kg","0.76"]
["","Náplň","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15"]
["Štandardné príslušenstvo","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Zdroj napájania","Frekvencia","","","Hz","50"]