{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","","","47","48"]
["","","","Men.","dBA","","52","","","49"]
["","Chladenie","","Vysoké","dBA","","","46","48"]
["","","","Men.","dBA","","52","","","49"]
["Štandardné príslušenstvo","Vypúšťacia skrutka","","","","","1","1","1","1"]
["","Návod na montáž","","","","","1","1","1","1"]
["","Štítok s náplňou chladiva","","","","","1","1","","1"]
["","Viacjazyčné štítky o fluórovaných skleníkových plynoch","","","","","1","1","","1"]
["Chladiace médium","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Náplň","","","kg","","1.70","1.0","1.2","1.50"]
["","Typ","","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot/min","","","780","780"]
["","","Kúrenie","Super nízke","ot/min","","","740","740"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Max.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","10","10","-10"]
["","Kúrenie","Okolitá teplota","Max.","°CWB","","18","18","18","18"]
["","","","Min.","°CWB","","-15","-15","-15","-15"]
["Pripojenia potrubia","Úroveň hladiny","IU - OU","Max.","m","","20.0","15","15","20.0"]
["","Dodatočná náplň chladiva","","","kg/m","","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["Úroveň akustického výkonu","Chladenie","","","dBA","","65","","","62"]
["","Vykurovanie","","","dBA","","65","","","62"]
["Kompresor","Typ","","","","","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","825","765","765","825"]
["","","","Hĺbka","mm","","300","285","285","300"]
["","","","Výška","mm","","735","550","550","735"]
["Hmotnosť","Jednotka","","","kg","","47","34","34","47"]
["Ventilátor","Prietok vzduchu","Kúrenie","Super nízke","cfm","","","904","904"]
["","","","Super nízke","m³/min","","","25.6","25.6"]
["","","Chladenie","Super nízke","m³/min","","","30.1","30.1"]
["","","","Super nízke","cfm","","","1,063","1,063"]
["Power supply","Fáza","","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","","50","50","50","50"]
["","Napätie","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Poznámky","","","","","(1) - 220 V","","(1) - Pri spojení s viacsystémovou vonkajšou jednotkou si preštudujte technické údaje viacsystémovej vonkajšej jednotky, ktorú chcete pripojiť.","(1) - Pri spojení s viacsystémovou vonkajšou jednotkou si preštudujte technické údaje viacsystémovej vonkajšej jednotky, ktorú chcete pripojiť."]
["","","","","","(2) - 230 V","","(2) - 220 V","(2) - 220 V"]
["","","","","","(3) - 240 V","","(3) - 230 V","(3) - 230 V"]
["","","","","","","","(4) - 240 V","(4) - 240 V"]
["","","","","","","","(5) - Obsahuje fluórované skleníkové plyny","(5) - Obsahuje fluórované skleníkové plyny"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","48.9"]
["","","Kúrenie","Super nízke","m³/min","43.1"]
["","","","Super nízke","cfm","1727"]
["","","Kúrenie","Super nízke","cfm","1522"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","735"]
["","","","Šírka","mm","825"]
["","","","Hĺbka","mm","300"]
["Hmotnosť","Jednotka","","","kg","47"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot/min","670"]
["","","Kúrenie","Super nízke","ot/min","670"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Kúrenie","Okolitá teplota","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","48"]
["","Kúrenie","","Vysoké","dBA","48"]
["Chladivo","Typ","","","","R-410A"]
["","Náplň","","","kg","1.7"]
["","Náplň","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","30"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","20"]
["Štandardné príslušenstvo","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Napájanie","Fáza","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50"]
["","Napätie","","","V","220-240"]
["Poznámky","","","","","","(1) - Obsahuje fluórované skleníkové plyny","","","(1) - Obsahuje fluórované skleníkové plyny"]