{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","","48"]
["","","","Nízka","dBA","","45"]
["Štandardné príslušenstvo","1","","","","","550"]
["Chladiace médium","Charge","","","kg","","2.5"]
["","Typ","","","","","1.2"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","","30.1"]
["","","","Super nízke","cfm","","1,063"]
["Motor ventilátora","Počet otáčok","Chladenie","Super nízke","ot./min.","","740"]
["","","Kúrenie","Super nízke","ot./min.","","-15"]
["Prevádzkový rozsah","Heating","Okolitá teplota","Min.","° CWB","","20"]
["","","","Max.","° CWB","","10"]
["Hladina akustického tlaku","Chladenie","","Nízka","dBA","","44"]
["","","","Vysoké","dBA","","48"]
["Kompresor","Typ","","","","","Hermeticky utesnený kolísavý kompresor"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","285"]
["","","","Hĺbka","mm","","612"]
["","","","Výška","mm","","765"]
["Hmotnosť","Jednotka","","","kg","","34"]
["Ventilátor","Prietok vzduchu","Kúrenie","Super nízke","cfm","","904"]
["","","","Super nízke","m³/min","","25.6"]
["Power supply","Phase","","","","","1~"]
["","Frekvencia","","","Hz","","50"]
["","Napätie","","","V","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - Obsahuje fluórované skleníkové plyny"]
["","","","","","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 230 V"]
["","","","","","","(4) - 240 V"]
["Ventilátor","Prietok vzduchu","Chladenie","Super nízke","m³/min","30.1"]
["","","Kúrenie","Super nízke","m³/min","25.6"]
["","","","Super nízke","cfm","1063"]
["","","Kúrenie","Super nízke","cfm","904"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","550"]
["","","","Šírka","mm","765"]
["","","","Hĺbka","mm","285"]
["Hmotnosť","Jednotka","","","kg","34"]
["Motor ventilátora","Rýchlosť","Chladenie","Super nízke","ot./min.","780"]
["","","Kúrenie","Super nízke","ot./min.","740"]
["Kompresor","Typ","","","","Hermeticky utesnený kolísavý kompresor"]
["Prevádzkový rozsah","Chladenie","Okolitá teplota","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Kúrenie","Okolitá teplota","Min.","° CWB","-15"]
["","","","Max.","° CWB","18"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","46"]
["","Kúrenie","","Vysoké","dBA","47"]
["","","","Nízka","dBA","44"]
["Chladivo","Typ","","","","R-410A"]
["","Náplň","","","kg","1.0"]
["","Náplň","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Pripojenia potrubí","Dĺžka potrubia","Max.","OU - IU","m","20"]
["","Dodatočná náplň chladiva","","","kg/m","0,02 (pre potrubie s dĺžkou presahujúcou 10m)"]
["","Úroveň hladiny","IU - OU","Max.","m","15"]
["Štandardné príslušenstvo","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Napájanie","Fáza","","","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50"]
["","Napätie","","","V","220-240"]