{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","","","","","","43"]
["","","","Stredný","dBA","","","","","","35"]
["","","","Tichá prevádzka","dBA","","","","","","26"]
["","","","Nízka","dBA","","","","","","29"]
["","Chladenie","","Stredný","dBA","","","","","","34"]
["","","","Tichá prevádzka","dBA","","","","","","20"]
["","","","Nízka","dBA","","","","","","27"]
["","","","Vysoké","dBA","","","","","","43"]
["Štandardné príslušenstvo","Návod na montáž","","","","","","","","","1"]
["","Návod na prevádzku","","","","","","","","","1"]
["","Infračervené diaľkové ovládanie","","","","","","","","","1"]
["","Batérie so suchými článkami typu AA","","","","","","","","","2"]
["","Držiak diaľkového ovládača","","","","","","","","","1"]
["","Montážna platnička","","","","","","","","","1"]
["","Titánovo apatitový fotokatalytický filter na čistenie vzduchu","","","","","","","","","2"]
["","Upevňovacie skrutky vnútornej jednotky","","","","","","","","","2"]
["Riadiace systémy","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Pripojenia potrubí","Kvapalina","","OD","mm","","","","","","6.35"]
["","Plyn","","OD","mm","","","","","","9.50"]
["","Vypúšťanie","","","","","","","","","18"]
["Príkon","Chladenie","","Men.","kW","","","","","","0.024"]
["","Kúrenie","","Men.","kW","","","","","","0.029"]
["Sound power level","Chladenie","","","dBA","","","","","","58"]
["","Vykurovanie","","","dBA","","","","","","58"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","","","","","770"]
["","","","Hĺbka","mm","","","","","","225"]
["","","","Výška","mm","","","","","","286"]
["Opláštenie","Farba","","","","","","","","","Biela"]
["Hmotnosť","Jednotka","","","kg","","","","","","9.0"]
["Power supply","Fáza","","","","","","","","","1~"]
["","Frekvencia","","","Hz","","","","","","50"]
["","Názov","","","","","","","","","V1"]
["","Napätie","","","V","","","","","","220-240"]
["Poznámky","","","","","","","","","","(1) - SL: Režim tichej prevádzky ventilátora s nastavením rýchlosti prietoku vzduchu"]
["Vstup napájania","Chladenie","","Men.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Kúrenie","","Men.","kW","0.022","0.022","0.023","0.023","0.029"]
["Opláštenie","Farba","","","","Biela","Biela","Biela","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","286","286","286","286","286"]
["","","","Šírka","mm","770","770","770","770","770"]
["","","","Hĺbka","mm","225","225","225","225","225"]
["Hmotnosť","Jednotka","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","","Stredný","m³/min","7.8","7.8","8","8","8.2"]
["","","","Nízka","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Tichá prevádzka","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Kúrenie","Vysoké","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","Vykurovanie","Stredný","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","Kúrenie","Nízka","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Tichá prevádzka","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Akustický výkon","Chladenie","","","dBA","55","55","55","55","58"]
["","Vykurovanie","","","dBA","55","55","55","55","58"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","39","39","40","40","43"]
["","","","Stredný","dBA","33","33","33","33","34"]
["","","","Nízka","dBA","25","25","26","26","27"]
["","","","Tichá prevádzka","dBA","20","20","20","20","20"]
["","Kúrenie","","Vysoké","dBA","39","39","40","40","43"]
["","Vykurovanie","","Stredný","dBA","34","34","34","34","35"]
["","Kúrenie","","Nízka","dBA","28","28","28","28","29"]
["","","","Tichá prevádzka","dBA","23","23","23","23","26"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Plyn","","OD","mm","9.5","9.5","9.5","9.5","9.5"]
["","Odvod kondenzátu","","","","18","18","18","18","18"]
["Riadiace systémy","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Štandardné príslušenstvo","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Napájanie","Názov","","","","V1","V1","V1","V1","V1"]
["","Fáza","","","","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50"]
["","Napätie","","","V","220-240","220-240","220-240","220-240","220-240"]
["Štandardné príslušenstvo","AAA dry-cell batteries","","","","","2","","2","2"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","","","ARC480A11","ARC480A11"]
["Štandardné príslušenstvo","Titanium apatite photocatalytic air purification filter","","","","","","2"]