{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","40","42","44","45"]
["","","","Stredný","dBA","34","38","40","41"]
["","","","Tichá prevádzka","dBA","21","30","32","33"]
["","","","Nízka","dBA","28","33","35","36"]
["","Chladenie","","Stredný","dBA","33","39","41","42"]
["","","","Tichá prevádzka","dBA","20","31","33","34"]
["","","","Nízka","dBA","26","34","36","37"]
["","","","Vysoké","dBA","40","43","45","46"]
["Štandardné príslušenstvo","Batérie so suchými článkami typu AAA","","","","2","2","2","2"]
["","Návod na montáž","","","","1","1","1","1"]
["","Návod na prevádzku","","","","1","1","1","1"]
["","Infračervené diaľkové ovládanie","","","","1","1","1","1"]
["","Držiak diaľkového ovládača","","","","1","1","1","1"]
["","Montážna platnička","","","","1","1","1","1"]
["","Upevňovacie skrutky vnútornej jednotky","","","","2","2","2","2"]
["Riadiace systémy","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Pripojenia potrubí","Kvapalina","","OD","mm","6.35","6.35","6.35","6.35"]
["","Plyn","","OD","mm","9.50","12.7","12.7","12.7"]
["","Vypúšťanie","","","","18","18","18","18"]
["Príkon","Chladenie","","Men.","kW","0.019","0.029","0.032","0.032"]
["","Kúrenie","","Men.","kW","0.020","0.032","0.035","0.035"]
["Sound power level","Chladenie","","","dBA","55","59","60","62"]
["","Vykurovanie","","","dBA","55","61","62","62"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","770","990","990","990"]
["","","","Hĺbka","mm","225","263","263","263"]
["","","","Výška","mm","286","295","295","295"]
["Opláštenie","Farba","","","","Biela","Biela","Biela","Biela"]
["Hmotnosť","Jednotka","","","kg","8.50","13.5","13.5","13.5"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","10.3","17.3","17.9","17.9"]
["","","","Nízka","m³/min","6.7","12.2","12.8","12.8"]
["","","","Stredný","m³/min","8.6","14.8","15.8","15.8"]
["","","","Tichá prevádzka","m³/min","5.3","10.7","11.3","11.3"]
["","","Chladenie","Nízka","m³/min","6.1","11.9","12.2","12.2"]
["","","","Stredný","m³/min","8.1","14.4","14.8","14.8"]
["","","","Vysoké","m³/min","10.1","16.8","17.3","17.3"]
["","","","Tichá prevádzka","m³/min","4.4","10.5","10.7","10.7"]
["Power supply","Fáza","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50","50","50","50"]
["","Názov","","","","","V1","V1","V1"]
["","Napätie","","","V","220-240","220-240","220-240","220-240"]
["Vstup napájania","Chladenie","","Men.","kW","","","","","0.019","0.032"]
["","Kúrenie","","Men.","kW","","","","","0.02","0.032"]
["Opláštenie","Farba","","","","","","","","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","","","","286","286"]
["","","","Šírka","mm","","","","","770","770"]
["","","","Hĺbka","mm","","","","","225","225"]
["Hmotnosť","Jednotka","","","kg","","","","","8.5","9"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","","","","10.1","11.5"]
["","","","Stredný","m³/min","","","","","8.1","8.3"]
["","","","Nízka","m³/min","","","","","6.1","6.3"]
["","","","Tichá prevádzka","m³/min","","","","","4.4","4.5"]
["","","Kúrenie","Vysoké","m³/min","","","","","10.3","11.5"]
["","","Vykurovanie","Stredný","m³/min","","","","","8.6","9"]
["","","Kúrenie","Nízka","m³/min","","","","","6.7","7"]
["","","","Tichá prevádzka","m³/min","","","","","5.3","5.3"]
["Akustický výkon","Chladenie","","","dBA","","","","","55","58"]
["","Vykurovanie","","","dBA","","","","","55","58"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","","","","40","43"]
["","","","Stredný","dBA","","","","","33","34"]
["","","","Nízka","dBA","","","","","26","27"]
["","","","Tichá prevádzka","dBA","","","","","20","20"]
["","Kúrenie","","Vysoké","dBA","","","","","40","40"]
["","Vykurovanie","","Stredný","dBA","","","","","34","35"]
["","Kúrenie","","Nízka","dBA","","","","","28","29"]
["","","","Tichá prevádzka","dBA","","","","","21","21"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","","","","6.35","6.35"]
["","Plyn","","OD","mm","","","","","9.5","9.5"]
["","Odvod kondenzátu","","","","","","","","18","18"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","","","","","ARC470A1","ARC470A1"]
["","Káblový diaľkový ovládač","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Štandardné príslušenstvo","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Napájanie","Fáza","","","","","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","","","","50","50"]
["","Napätie","","","V","","","","","220-240","220-240"]