{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-G"]
[]
[]
[]
[]
["","","","","","ATXF25G5V1B","ATXF35G5V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.023","0.029"]
["","Kúrenie","","Men.","kW","0.023","0.023"]
["Opláštenie","Farba","","","","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","286","286"]
["","","","Šírka","mm","770","770"]
["","","","Hĺbka","mm","225","225"]
["Hmotnosť","Jednotka","","","kg","8.5","9"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","9.8","10.9"]
["","","","Stredný","m³/min","8","7"]
["","","","Nízka","m³/min","6","5.7"]
["","","","Tichá prevádzka","m³/min","4.3","4.6"]
["","","Kúrenie","Vysoké","m³/min","10.4","9.3"]
["","","Vykurovanie","Stredný","m³/min","8.4","7.5"]
["","","Kúrenie","Nízka","m³/min","6.4","6"]
["","","","Tichá prevádzka","m³/min","5.3","5.2"]
["Akustický výkon","Chladenie","","","dBA","54","54"]
["","Vykurovanie","","","dBA","55","56"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","40","56"]
["","","","Stredný","dBA","33"]
["","","","Nízka","dBA","26"]
["","","","Tichá prevádzka","dBA","20"]
["","Kúrenie","","Vysoké","dBA","40","40"]
["","Vykurovanie","","Stredný","dBA","34","35"]
["","Kúrenie","","Nízka","dBA","28","29"]
["","","","Tichá prevádzka","dBA","21","21"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6","6"]
["","Plyn","","OD","mm","9.5","9.5"]
["","Odvod kondenzátu","","","","18","18"]
["Riadiace systémy","Infra. diaľkové ovládanie","","","","ARC480A93","ARC480A93"]
["","Káblový diaľkový ovládač","","","","BRC073A1","BRC073A1"]
["Štandardné príslušenstvo","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Napájanie","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-440","220-440"]
["Poznámky","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 5m; výškový rozdiel: 0m","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 5m; výškový rozdiel: 0m"]
["","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m (horizontálna)","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 5m (horizontálna)"]
["","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch","(3) - Elektrické údaje nájdete v samostatných nákresoch"]