{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-K3 / ARXP-K3"]
[]
[]
[]
[]
["","","","","ATXP20K3V1B / ARXP20K3V1B","ATXP25K3V1B / ARXP25K3V1B","ATXP35K3V1B / ARXP35K3V1B"]
["Chladiaci výkon","Men.","","kW","","2.50","3.50"]
["Nominálna účinnosť","EER","","","","3.79","3.45"]
["","COP","","","","4.36","4.02"]
["","Smernica o energetickom označovaní","Chladenie","","","A","A"]
["","","Vykurovanie","","","A","A"]
["Vykurovací výkon","Men.","","kW","","3.00","4.00"]
["Poznámky","","","","","(1) - Chladenie: T2: vnútorná teplota 26,6°CDB, 19,4°CWB, vonk. tepl. 48°CDB [Btu/h/W]","(1) - Chladenie: T2: vnútorná teplota 26,6°CDB, 19,4°CWB, vonk. tepl. 48°CDB [Btu/h/W]"]
["","","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["","","","","","(3) - Elektrické údaje nájdete v samostatných nákresoch","(3) - Elektrické údaje nájdete v samostatných nákresoch"]
["Vonkajšia jednotka","","","","ARXP20K3V1B"]
["Chladiaci výkon","Men.","","kW","2.00"]
["Vykurovací výkon","Men.","","kW","2.50"]
["Nominálna účinnosť","EER","","","3.98"]
["","COP","","","4.77"]
["","Smernica o energetickom označovaní","Chladenie","","A"]
["","","Vykurovanie","","A"]
["Chladenie","Trieda energetickej účinnosti","","","A++"]
["","Výkon","P návrh","kW","2.00"]
["","SEER","","","6.75"]
["","Ročná spotreba energie","","kWh/a","104"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A++"]
["","Výkon","P návrh","kW","2.20"]
["","SCOP/A","","","4.64"]
["","Pdh Vykurovací výkon pri -10°","","kW","2.19"]
["","Ročná spotreba energie","","kWh/a","664"]