{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Použitie","","","","","Parapetný typ"]
["Výkon","m³/min","","","","33.33"]
["Opláštenie","Farba","","","","Natretý pozinkovaný plech"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","1628"]
["","","","Šírka","mm","720"]
["","","","Hĺbka","mm","770"]
["Hmotnosť","Jednotka","","","kg","150"]
["Použiteľná oblasť v miestnosti","m²","","","","133"]
["Prevádzka čističky vzduchu","Vstup napájania","","H","kW","0.379"]
["Hladina akustického tlaku","Prevádzka čističky vzduchu","","Vysoké","dBA","55.9"]
["Ventilátor","Prietok vzduchu","Prevádzka čističky vzduchu","Turbo","m³/h","2300"]
["","","","Vysoké","m³/h","2000"]
["Bezpečnostné zariadenia","Položka","","01","","Bezpečnostný spínač (činnosť sa zastaví, keď sú otvorené zadné dvierka)"]
["Štandardné príslušenstvo","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Napájací kábel","m","","","","3"]
["Zdroj napájania","Frekvencia","","","Hz","50/60"]
["Prevádzkový prúd","Prevádzka čističky vzduchu","","Vysoké","A","1.73"]