{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32","CHYHBH05AFV32","CHYHBH08AFV32"]
["Opláštenie","Farba","","","","Biela","Biela","Biela"]
["","Materiál","","","","Predobalený tabuľový plech","Predobalený tabuľový plech","Predobalený tabuľový plech"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","902","902","902"]
["","","","Šírka","mm","450","450","450"]
["","","","Hĺbka","mm","164","164","164"]
["Hmotnosť","Jednotka","","","kg","30.0","30.0","30.0"]
["PED","Kategória","","","","","Art3§3, Vylúčená z rozsahu PED kvôli článku 1, položka 3.6 Smernice 97/23/ES","Art3§3, Vylúčená z rozsahu PED kvôli článku 1, položka 3.6 Smernice 97/23/ES"]
["Výmenník tepla na strane vody","Rýchlosť prietoku vody","Kúrenie","Max.","l/min","23.0 (5)","23.0 (5)","23.0 (5)"]
["Úroveň akustického výkonu","Men.","","","dBA","42 (6)","42 (6)","42 (6)"]
["Prevádzkový rozsah","Kúrenie","Strana vody","Min.","°C","25 (7)","25 (7)","25 (7)"]
["","","","Max.","°C","50 (7)","50 (7)","50 (7)"]
["Napájanie","Názov","","","","V3","V3","V3"]
["","Fáza","","","","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50"]
["","Napätie","","","V","230","230","230"]
["Pripojenia vedenia","Pripojenia vedenia-=-Na prepojenie s&nbsp;používateľským rozhraním","","Pripojenia vedenia-=-Na prepojenie s&nbsp;používateľským rozhraním-=-Množstvo","","2","2","2"]
["","","","Pripojenia vedenia-=-Na prepojenie s&nbsp;používateľským rozhraním-=-Poznámka","","0,75 mm² až do 1,25 mm² (max. dĺžka 500 m)","0,75 mm² až do 1,25 mm² (max. dĺžka 500 m)","0,75 mm² až do 1,25 mm² (max. dĺžka 500 m)"]
["Poznámky","","","","","(1) - Len pre vnútornú jednotku","(1) - Len pre vnútornú jednotku","(1) - Len pre vnútornú jednotku"]
["","","","","","(2) - DB/WB 7°C/6°C – LWC 35°C (DT=5°C), kotol obídený","(2) - DB/WB 7°C/6°C – LWC 35°C (DT=5°C), kotol obídený","(2) - DB/WB 7°C/6°C – LWC 35°C (DT=5°C), kotol obídený"]
["","","","","","(3) - DB/WB 7°C/6°C – LWC 45°C (DT=5°C), kotol obídený","(3) - DB/WB 7°C/6°C – LWC 45°C (DT=5°C), kotol obídený","(3) - DB/WB 7°C/6°C – LWC 45°C (DT=5°C), kotol obídený"]
["","","","","","(4) - Min. required","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Kotol obídený","(5) - Kotol obídený","(5) - Kotol obídený"]
["","","","","","(6) - Podľa normy EN14825","(6) - Podľa normy EN14825","(6) - Podľa normy EN14825"]
["","","","","","(7) - Prevádzkový rozsah jednotiek *HYHB* a *HYKOMB33AA nájdete na nákrese prevádzkového rozsahu","(7) - Prevádzkový rozsah jednotiek *HYHB* a *HYKOMB33AA nájdete na nákrese prevádzkového rozsahu","(7) - Prevádzkový rozsah jednotiek *HYHB* a *HYKOMB33AA nájdete na nákrese prevádzkového rozsahu"]