{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BB"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BB"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","39"]
["","","","Stredný","dBA","32"]
["","","","Tichá prevádzka","dBA","21"]
["","","","Nízka","dBA","25"]
["","Chladenie","","Stredný","dBA","32"]
["","","","Tichá prevádzka","dBA","21"]
["","","","Nízka","dBA","25"]
["","","","Vysoké","dBA","39"]
["Štandardné príslušenstvo","Návod na montáž","","","","1"]
["","Návod na prevádzku","","","","1"]
["","Vzduchový filter","","","","2"]
["","Infračervené diaľkové ovládanie","","","","1"]
["","Montážna platnička diaľkového ovládača","","","","1"]
["","Nádobka na skrutky","","","","1"]
["","Kryt na skrutky","","","","2"]
["","Batérie so suchými článkami typu AAA","","","","2"]
["","Všeobecné bezpečnostné opatrenia","","","","1"]
["Chladiace médium","GWP","","","","675.0"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","BRC073"]
["","Infra. diaľkové ovládanie","","","","ARC466A58"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35"]
["","Plyn","","OD","mm","9.50"]
["","Vypúšťanie","","","","18"]
["Vstup napájania","Chladenie","","Men.","kW","0.020"]
["","Kúrenie","","Men.","kW","0.020"]
["Akustický výkon","Chladenie","","","dBA","57"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","798"]
["","","","Hĺbka","mm","189"]
["","","","Výška","mm","295"]
["Opláštenie","Farba","","","","Čierna"]
["Hmotnosť","Jednotka","","","kg","11.5"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","10.9"]
["","","","Stredný","m³/min","8.7"]
["","","","Nízka","m³/min","6.4"]
["","","","Tichá prevádzka","m³/min","4.5"]
["","","Chladenie","Nízka","m³/min","6.1"]
["","","","Stredný","m³/min","8.2"]
["","","","Vysoké","m³/min","11.0"]
["","","","Tichá prevádzka","m³/min","4.6"]
["Power supply","Fáza","","","","1~"]
["","Názov","","","","V1"]
["","Frekvencia","","","Hz","50"]
["","Napätie","","","V","220-240"]