{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Vstup napájania","Chladenie","","Men.","kW","0.029","0.029"]
["","Kúrenie","","Men.","kW","0.023","0.023"]
["Opláštenie","Farba","","","","Biela","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","295","295"]
["","","","Šírka","mm","778","778"]
["","","","Hĺbka","mm","272","272"]
["Hmotnosť","Jednotka","","","kg","10","10"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","10.5","10.5"]
["","","","Stredný","m³/min","7.5","7.5"]
["","","","Nízka","m³/min","5.7","5.7"]
["","","","Tichá prevádzka","m³/min","4.3","4.3"]
["","","Kúrenie","Vysoké","m³/min","9.3","9.3"]
["","","Vykurovanie","Stredný","m³/min","8.2","8.2"]
["","","Kúrenie","Nízka","m³/min","6.2","6.2"]
["","","","Tichá prevádzka","m³/min","5.1","5.1"]
["Akustický výkon","Chladenie","","","dBA","57","57"]
["","Vykurovanie","","","dBA","54","54"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","41","41"]
["","","","Stredný","dBA","33","33"]
["","","","Nízka","dBA","25","25"]
["","","","Tichá prevádzka","dBA","19","19"]
["","Kúrenie","","Vysoké","dBA","39","39"]
["","Vykurovanie","","Stredný","dBA","34","34"]
["","Kúrenie","","Nízka","dBA","26","26"]
["","","","Tichá prevádzka","dBA","20","20"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35"]
["","Plyn","","OD","mm","9.5","9.5"]
["","Odvod kondenzátu","","","","18","18"]
["Riadiace systémy","Infrared remote control","","","","ARC466A67","ARC466A67"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","BRC073A1","BRC073A1"]
["Štandardné príslušenstvo","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Napájanie","Názov","","","","V1","V1"]
["","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]