{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Hladina akust. tlaku","Kúrenie","","Vysoké","dBA","38","","41"]
["","","","Tichá prevádzka","dBA","21","","21"]
["","","","Nízka","dBA","28","","30"]
["","Chladenie","","Tichá prevádzka","dBA","21","","21"]
["","","","Nízka","dBA","25","","28"]
["","","","Vysoké","dBA","37","","42"]
["","","","Men.","dBA","33"]
["","Chladenie","","Men.","dBA","31","","35"]
["Štandardné príslušenstvo","Návod na montáž","","","","1","","1"]
["","Návod na prevádzku","","","","1","","1"]
["","Bezdrôtové diaľkové ovládanie","","","","1","","1"]
["","Batérie","","","","2","","2"]
["","Držiak diaľkového ovládača","","","","1","","1"]
["","Montážna platnička","","","","1","","1"]
["","Upevňovacie skrutky vnútornej jednotky","","","","2","","2"]
["","Titánovo apatitový fotokatalytický filter na čistenie vzduchu","","","","2","","2"]
["Riadiace systémy","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","","6.35"]
["","Plyn","","OD","mm","9.5","","9.5"]
["","Vypúšťanie","","","","18","","18"]
["Vstup napájania","Chladenie","","Men.","kW","0.040","","0.040"]
["","Kúrenie","","Men.","kW","0.040","","0.040"]
["Úroveň akustického výkonu","Chladenie","","","dBA","55","","59"]
["","Vykurovanie","","","dBA","56","","58"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","780","","780"]
["","","","Hĺbka","mm","215","","215"]
["","","","Výška","mm","289","","289"]
["Kryt","Farba","","","","Biela","","Biela"]
["Hmotnosť","Jednotka","","","kg","8","","8"]
["Ventilátor","Prietok vzduchu","Kúrenie","Vysoké","m³/min","","","10.1"]
["","","","Nízka","m³/min","","","6.3"]
["","","","Tichá prevádzka","m³/min","","","4.3"]
["","","Chladenie","Nízka","m³/min","","","5.2"]
["","","","Vysoké","m³/min","","","9.2"]
["","","","Tichá prevádzka","m³/min","","","3.9"]
["","","","Men.","m³/min","","","8.1"]
["","","Chladenie","Men.","m³/min","","","7.2"]
["Power supply","Fáza","","","","1~","","1~"]
["","Frekvencia","","","Hz","50","","50"]
["","Názov","","","","V1","","V1"]
["","Napätie","","","V","220-240","","220-240"]
["Poznámky","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Vstup napájania","Chladenie","","Men.","kW","","0.04","","0.040"]
["","Kúrenie","","Men.","kW","","0.04","","0.040"]
["Opláštenie","Farba","","","","","Biela","","Biela"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","","289","","289"]
["","","","Šírka","mm","","780","","780"]
["","","","Hĺbka","mm","","215","","215"]
["Hmotnosť","Jednotka","","","kg","","8","","8.00"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","","7.9","","9.2"]
["","","","Stredný","m³/min","","6.3","","7.2"]
["","","","Nízka","m³/min","","4.7","","5.2"]
["","","","Tichá prevádzka","m³/min","","3.9","","3.9"]
["","","Kúrenie","Vysoké","m³/min","","9","","10.1"]
["","","Vykurovanie","Stredný","m³/min","","7.5","","8.1"]
["","","Kúrenie","Nízka","m³/min","","6","","6.3"]
["","","","Tichá prevádzka","m³/min","","4.3","","4.3"]
["Akustický výkon","Chladenie","","","dBA","","55","","59"]
["","Vykurovanie","","","dBA","","56","","58"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","","37","","42"]
["","","","Stredný","dBA","","31","","35"]
["","","","Nízka","dBA","","25","","28"]
["","","","Tichá prevádzka","dBA","","21","","21"]
["","Kúrenie","","Vysoké","dBA","","38","","41"]
["","Vykurovanie","","Stredný","dBA","","33","","36"]
["","Kúrenie","","Nízka","dBA","","28","","30"]
["","","","Tichá prevádzka","dBA","","21","","21"]
["Pripojenia potrubia","Kvapalina","","OD","mm","","6.35","","6.35"]
["","Plyn","","OD","mm","","9.5","","9.50"]
["","Odvod kondenzátu","","","","","18","","18"]
["Riadiace systémy","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Štandardné príslušenstvo","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Napájanie","Názov","","","","","V1","","V1"]
["","Fáza","","","","","1~","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","","50","","50"]
["","Napätie","","","V","","220-240","","220-240"]