{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":11,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","D2CND-A4A"]
[]
[]
[]
[]
["","","","","","D2CND024A4AB","D2CND024A4AA","D2CND028A4AA","D2CND028A4AB","D2CND035A4AA","D2CND035A4AB"]
["Plyn","Spotreba (G20)","","Min","m³/h","0.31","0.31","0.511","0.511","0.511","0.511"]
["","","","Max","m³/h","2.48","2.48","2.89","2.89","3.63","3.63"]
["","Spotreba (G25)","","Min","m³/h","0.36","0.36","0.59","0.59","0.59","0.59"]
["","","","Max","m³/h","2.89","2.89","3.32","3.32","4.19","4.19"]
["","Spotreba (G31)","","Min","m³/h","0.12","0.12","0.2","0.2","0.2","0.2"]
["","","","Max","m³/h","0.96","0.96","1.1","1.1","1.38","1.38"]
["","Trieda NOx","","","","6","6","6","6","6","6"]
["","Úroveň NOx (G20)","","","mg/kWh","22","22","36.3","36.3","35.5","35.5"]
["Centrálne vykurovanie","Tepelný výkon Qn (čistá kalorifická hodnota)","Nom. ot.","Min","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Centrálne vykurovanie-=-Tepelný výkon Qn (čistá kalorifická hodnota)-=-Nom. ot.-=-Max-=-kW","kW","23.5","23.5","27","27","34","34"]
["","Tepelný výkon Qn (hrubá kalorifická hodnota)","Nom. ot.","Min","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max","kW","26.1","26.1","30","30","37.8","37.8"]
["","Výkon Pn pri 80/60°C","","Min","kW","2.8","2.8","4.6","4.6","4.6","4.6"]
["","","","Nom. ot.","kW","22.8","22.8","26.3","26.3","33.2","33.2"]
["","Výkon Pnc pri 50/30°C","","Min","kW","3.1","3.1","5.2","5.2","5.2","5.2"]
["","","","Nom. ot.","kW","24","24.0","28.2","28.2","35","35"]
["","Výkon pri 37/30°C","","Nom. ot.","kW","7.6","7.6","8.8","8.8","11.1","11.1"]
["","Teplota vody","","Max","°C","100","100","100","100","100","100"]
["","Účinnosť","","Čistá kalorifická hodnota","%","97.9","97.9"]
["","","","Hrubá kalorifická hodnota","%","87.3","87.3"]
["Teplá pitná voda","Tepelný výkon (čistá kalorifická hodnota) Qnw","Nom. ot.","Min","kW","2.9","2.9","4.8","4.8","4.8","4.8"]
["","","","Max","kW","23.5","23.5","29.5","29.5","34","34"]
["","Tepelný výkon (hrubá kalorifická hodnota) Qnw","Nom. ot.","Min","kW","3.2","3.2","5.3","5.3","5.3","5.3"]
["","","","Max","kW","26.1","26.1","32.7","32.7","37.7","37.7"]
["","Teplota","","Max","°C","60","60","60","60","60","60"]
["Tepelné straty","Záložný kotol Ps","","","kW","0.057","0.057","0.0650","0.065","0.0650","0.065"]
["Privádzaný vzduch","Pripojenie","","","mm","100","100","100","100","100","100"]
["","Koncentrické","","","","Áno","Áno","Áno","Áno","Áno","Áno"]
["Dymový plyn","Teplota","","Max","°C","90","90","76.4","76.4","81.7","81.7"]
["","Pripojenie","","","mm","60","60","60","60","60","60"]
["","Hmotnostný prietok (G20)","","Max","kg/h","38.7","38.7","44.5","55.7","55.7","55.7"]
["","Hmotnostný prietok (G31)","","Max","kg/h","36","36.0","43.3","43.3","54.7","54.7"]
["Opláštenie","Farba","","","","Titániovo biela (Ral9003)","Titániovo biela (Ral9003)","Titániovo biela (Ral9003)","Titániovo biela (Ral9003)","Titániovo biela (Ral9003)","Titániovo biela (Ral9003)"]
["","Materiál","","","","Oceľový plech","Oceľový plech","Galvanizovaný oceľový plech s práškovou povrchovou úpravou","Galvanizovaný oceľový plech s práškovou povrchovou úpravou","Galvanizovaný oceľový plech s práškovou povrchovou úpravou","Galvanizovaný oceľový plech s práškovou povrchovou úpravou"]
["Vonkajšie rozmery","Jednotka","Výška","Opláštenie","mm","590","590","690","690","690","690"]
["","","","Šírka","mm","400","400","440","440","440","440"]
["","","","Hĺbka","mm","256","256","295","295","295","295"]
["Hmotnosť","Jednotka","","Prázdna","kg","27","27","37","37","37","37"]
["","","","Plná","kg","27","27","39","","39"]
["","Kotol","","Prázdna","kg","27","27.0"]
["Ohrev teplej pitnej vody","Všeobecné","","Uvedený záťažový profil","","XL","XL","XL","XL","XL","XL"]
["","","","Trieda energetickej účinnosti ohrevu vody","","A","A","A","A","A","A"]
["Vykurovanie priestoru","Všeobecné","","Trieda sezónnej účinnosti vykurovania priestoru","","A","A","A","A","A","A"]
["Dymový plyn","Hmotnostný prietok (G25)","","Max","kg/h","","","39.3","39.3","49.6","49.6"]