{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Príkon","kW","","","","0.015"]
["Maximálny počet pripojiteľných vnútorných jednotiek","","","","","32"]
["Maximálny počet pripojiteľných vonkajších jednotiek @","","","","","7"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","136"]
["","","","Šírka","mm","384"]
["","","","Hĺbka","mm","92"]
["Komunikácia","DIII-NET","","Množstvo","","1"]
["","","","Poznámka","","DIII-NET (F1F2)"]
["","Ethernet","","Množstvo","","1"]
["","Vstupný terminál","Digitálny","Množstvo","","4"]
["teplota vonkajšieho prostredia","Prevádzka","","Min.","°C","-10"]
["","","","Max.","°C","50"]
["","Uskladnenie","","Min.","°C","-20"]
["","","","Max.","°C","60"]
["Teplota prostredia","Teplota prostredia-=-Relatívna vlhkosť <-=-%","","","%","85"]
["Zdroj napájania","Frekvencia","","","Hz","50/60"]
["","Napätie","","","V","110-240 AC"]
["Poznámky","","","","","(1) - Zahrňuje príkon napájania WAGO, modulu CPU a modulu I/O"]
["","","","","","(2) - Rozmery zahrňujú napájanie WAGO, modul CPU, modul I/O a potrebný priestor medzi rôznymi dielmi"]
["","","","","","(3) - Rozmery voliteľnej obrazovky sú: výška: 209 mm, šírka: 123 mm, hĺbka: 8,5 mm"]