{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Hladina akustického tlaku","Men.","","","dBA","32.0 (6)"]
["Chladiace médium","GWP","","","","2,090"]
["","Náplň","","","kg","1.80"]
["","Type","","","","R-410A"]
["Prevádzkový rozsah","Inštalačný priestor","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Heating","Strana vody","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Solanková strana","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Teplá úžitková voda","Strana vody","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Vstup napájania","Men.","","","kW","2.38 (1), 2.89 (2)"]
["Akustický výkon","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","600"]
["","","","Hĺbka","mm","728"]
["","","","Výška","mm","1,730"]
["Casing","Material","","","","Predobalený tabuľový plech"]
["","Farba","","","","Biela"]
["Zásobník","Objem vody","","","l","180"]
["","Ochrana proti korózii","","","","Anóda"]
["","Izolácia","","Tepelná strata","kWh/24h","1.36 (4)"]
["Hmotnosť","Jednotka","","","kg","210"]
["Vykur. priestoru","Priem. podnebie – výstup vody 35°C","Všeobecné","ηs (Sezónna účinnosť vykurovania priestoru)","%","194"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A+++"]
["","","","SCOP","","5.06"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++"]
["","","","ηs (Sezónna účinnosť vykurovania priestoru)","%","139"]
["","","","SCOP","","3.68"]
["Vykurovací výkon","Men.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Phase","","","","3~"]
["","Názov","","","","9W"]
["","Frekvencia","","","Hz","50"]
["","Napätie","","","V","400"]
["Current","Recommended fuses","","","A","25"]
["Poznámky","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45°C (DT=5°C)"]
["","","","","","(3) - so 40% propylénglykolu"]
["","","","","","(4) - Tepelná strata podľa normy EN12897"]
["","","","","","(5) - Vrátane potrubia + PHE + záložný ohrievač; bez expanznej nádoby"]
["","","","","","(6) - Hladina tlaku zvuku sa meria mikrofónom vo vzdialenosti 1 m od jednotky. Predstavuje relatívnu hodnotu závislú od vzdialenosti a akustiky."]
["","","","","","(7) - Tepelným čerpadlom"]
["","","","","","(8) - Tepelným čerpadlom + záložným ohrievačom"]
["","","","","","(9) - Záložným ohrievačom"]