{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSXB-E"]
[]
[]
[]
[]
["","","","","","EHSXB04P30EG","EHSXB04P50EG","EHSXB08P30EG","EHSXB08P50EG","EHSXB04P30EF (Archived)","EHSXB04P50EF (Archived)","EHSXB08P30EF (Archived)","EHSXB08P50EF (Archived)"]
["Opláštenie","Farba","","","","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)"]
["","Materiál","","","","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","1891","1910","1891","1910","1892","1905","1892","1905"]
["","","","Šírka","mm","594","792","594","792","594","792","594","792"]
["","","","Hĺbka","mm","644","817","644","817","644","812","644","812"]
["Hmotnosť","Jednotka","","","kg","80.0","104","80.0","104","79","110","79","110"]
["PED","Kategória","","","","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3","Čl. 4.3"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0","675","675","675","675"]
["","Náplň","","","kg","1.50","1.50","1.50","1.50","1.5","1.5","1.5","1.5"]
["Úroveň akustického výkonu","Men.","","","dBA","39","39","39","39","39","39","39","39"]
["Prevádzkový rozsah","Kúrenie","Strana vody","Min.","°C","18","18","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65","65","65"]
["","Chladenie","Okolitá teplota","Min.","°CDB","10","10","10","10","10","10","10","10"]
["","","Strana vody","Min.","°C","5","5","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22","22","22"]
["Napájanie","Fáza","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50","50","50","50","50"]
["","Napätie","","","V","230","230","230","230","230","230","230","230"]
["Poznámky","","","","","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897"]