{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-UE6V / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHVH08SU18EA6V / ERGA08EAV3H7","EHVH08SU18EJ6V / ERGA08EAV3H7","EHVH08SU23EA6V / ERGA08EAV3H7","EHVH08SU23EJ6V / ERGA08EAV3H7"]
["Vykurovací výkon","Men.","","","kW","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Vstup napájania","Kúrenie","","Men.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["Príkon","Teplá pitná voda od 10°C do 50°C","","Nom. ot.","kWh","2.48","2.48","3.01","3.01"]
["Doba ohrevu od 10°C do 50°C","hod.","","","","1h 28 min","1h 28 min","1 h 40 min","1 h 40 min"]
["COP","","","","","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Ohrev teplej pitnej vody","Všeobecné","","Uvedený záťažový profil","","L","L","XL","XL"]
["","Priemerná klíma","","Trieda energetickej účinnosti ohrevu vody","","A+","A+","A+","A+"]
["Vykur. priestoru","Priemerné podnebie – výstup vody 55°C","Všeobecné","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A++","A++","A++","A++"]
["","Priemerné podnebie – výstup vody 35°C","Všeobecné","SCOP","","4.56","4.56","4.56","4.56"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A+++","A+++","A+++","A+++"]
["Rozsah energetickej účinnosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Poznámky","","","","","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)"]