{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-CB / ERHQ-BW1"]
[]
[]
[]
[]
["","","","","","EHVX11S18CB3V / ERHQ011BAW1","EHVX11S26CB9W / ERHQ011BAW1","EHVX16S18CB3V / ERHQ014BAW1","EHVX16S26CB9W / ERHQ014BAW1","EHVX16S18CB3V / ERHQ016BAW1","EHVX16S26CB9W / ERHQ016BAW1"]
["Ohrev tep. vody","Všeobecné","","Uvedený záťažový profil","","L","XL","L","","L","XL"]
["","Priemerná klíma","","Trieda energetickej účinnosti ohrevu vody","","A","A","A","","A","A"]
["COP","","","","","4.30 (1), 3.39 (2)","4.30 (1), 3.39 (2)","4.24 (1), 3.22 (2)","4.24, 3.22","4.20 (1), 3.22 (2)","4.20 (1), 3.22 (2)"]
["Chladiaci výkon","Men.","","","kW","15.1 (1), 11.7 (2)","15.1 (1), 11.7 (2)","16.1 (1), 12.6 (2)","","16.8 (1), 13.1 (2)","16.8 (1), 13.1 (2)"]
["EER","","","","","3.32 (1), 2.72 (2)","3.32 (1), 2.72 (2)","2.96 (1), 2.47 (2)","2.96, 2.47","2.72 (1), 2.29 (2)","2.72 (1), 2.29 (2)"]
["Vykurovací výkon","Men.","","","kW","11.3 (1), 11.0 (2)","11.3 (1), 11.0 (2)","14.5 (1), 13.6 (2)","","16.1 (1), 15.1 (2)","16.1 (1), 15.1 (2)"]
["Vstup napájania","Chladenie","","Men.","kW","4.53 (1), 4.31 (2)","4.53 (1), 4.31 (2)","5.43 (1), 5.08 (2)","","6.16 (1), 5.73 (2)","6.16 (1), 5.73 (2)"]
["","Kúrenie","","Men.","kW","2.63 (1), 3.24 (2)","2.63 (1), 3.24 (2)","3.42 (1), 4.21 (2)","","3.82 (1), 4.69 (2)","3.82 (1), 4.69 (2)"]
["Poznámky","","","","","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)"]
["","","","","","(3) - Tamb 35 °C - LWE 7 °C (DT = 5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT = 5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT = 5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT = 5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT = 5 °C)","(3) - Tamb 35 °C - LWE 7 °C (DT = 5 °C)"]
["","","","","","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)","(4) - Tamb 35°C - LWE 18℃ (DT=5°C)"]
["","","","","","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)","(5) - DB/WB 7°C/6°C-LWC 35°C(DT=5°C)"]
["","","","","","(6) - DB/WB 7 °C/6 °C - LWC 45 °C (Dt = 5 °C)","(6) - DB/WB 7 °C/6 °C - LWC 45 °C (Dt = 5 °C)","(6) - DB/WB 7 °C/6 °C - LWC 45 °C (Dt = 5 °C)","(6) - DB/WB 7 °C/6 °C - LWC 45 °C (Dt = 5 °C)","(6) - DB/WB 7 °C/6 °C - LWC 45 °C (Dt = 5 °C)","(6) - DB/WB 7 °C/6 °C - LWC 45 °C (Dt = 5 °C)"]
["Vykurovací výkon","Men.","","","kW","","","","14.5, 13.6"]
["Chladiaci výkon","Men.","","","kW","","","","16.1, 12.6"]
["Vstup napájania","Kúrenie","","Men.","kW","","","","3.42, 4.21"]
["","Chladenie","","Men.","kW","","","","5.43, 5.08"]
["Ohrev teplej pitnej vody","Všeobecné","","Uvedený záťažový profil","","","","","XL"]
["","Priemerná klíma","","Trieda energetickej účinnosti ohrevu vody","","","","","A"]
["Vykur. priestoru","Priemerné podnebie – výstup vody 55°C","Všeobecné","SCOP","","","","","2.80"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","","","","A+"]
["","Priemerné podnebie – výstup vody 35°C","Všeobecné","SCOP","","","","","3.34"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","","","","A+"]