{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-CB3V / ERHQ-BV3"]
[]
[]
[]
[]
["","","","","","EHVZ16S18CB3V / ERHQ011BAV3","EHVZ16S18CB3V / ERHQ014BAV3","EHVZ16S18CB3V / ERHQ016BAV3"]
["Vykurovací výkon","Men.","","","kW","11.2, 10.3","14.0, 13.1","16.0, 15.2"]
["Vstup napájania","Kúrenie","","Men.","kW","2.55, 3.17","3.26, 4.04","3.92, 4.75"]
["COP","","","","","4.39, 3.25","4.29, 3.24","4.08, 3.20"]
["Ohrev teplej pitnej vody","Všeobecné","","Uvedený záťažový profil","","L","L","L"]
["","Priemerná klíma","","Trieda energetickej účinnosti ohrevu vody","","A","A","A"]
["Vykur. priestoru","Priemerné podnebie – výstup vody 55°C","Všeobecné","SCOP","","2.86","2.82","2.92"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A+","A+","A+"]
["","Priemerné podnebie – výstup vody 35°C","Všeobecné","SCOP","","2.99","3.23","3.29"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A++","A+","A+"]
["Rozsah energetickej účinnosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Poznámky","","","","","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)","(1) - Stav 1: chladenie Ta 35 °C - LWE 18 °C (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)","(2) - Stav 2: chladenie Ta 35 °C - LWE 7℃ (DT = 5 °C); kúrenie Ta DB/WB 7 °C/6 °C – LWC 45℃ (DT = 5 °C)"]
["","","","","","","(3) - Výkon sa musí rozdeliť medzi prídavnú a hlavnú zónu. V údajoch ESP nájdete viac podrobností o dostupnej hlave (kPa).","(3) - Výkon sa musí rozdeliť medzi prídavnú a hlavnú zónu. V údajoch ESP nájdete viac podrobností o dostupnej hlave (kPa)."]