{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":11,"n_cols":7,"rows_kept":11,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBRD-ACV1 / ERRQ-AV1"]
[]
[]
[]
[]
["","","","","EKHBRD011ACV1 / ERRQ011AAV1","EKHBRD014ACV1 / ERRQ014AAV1","EKHBRD016ACV1 / ERRQ016AAV1"]
["COP","","","","3.08 (1), 2.50 (2)","3.00 (1), 2.48 (2)","2.88 (1), 2.41 (2)"]
["Vykurovací výkon","Men.","","kW","11 (1), 11 (2)","14 (1), 14 (2)","16 (1), 16 (2)"]
["Vstup napájania","Kúrenie","Men.","kW","3.57 (1), 4.40 (2)","4.66 (1), 5.65 (2)","5.57 (1), 6.65 (2)"]
["Poznámky","","","","(1) - EW 55°C; LW 65°C; Dt 10°C; okolité podmienky: 7°CDB/6°CWB","(1) - EW 55°C; LW 65°C; Dt 10°C; okolité podmienky: 7°CDB/6°CWB","(1) - EW 55°C; LW 65°C; Dt 10°C; okolité podmienky: 7°CDB/6°CWB"]
["","","","","(2) - EW 70°C; LW 80°C; Dt 10°C; okolité podmienky: 7°CDB/6°CWB","(2) - EW 70°C; LW 80°C; Dt 10°C; okolité podmienky: 7°CDB/6°CWB","(2) - EW 70°C; LW 80°C; Dt 10°C; okolité podmienky: 7°CDB/6°CWB"]