{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWCB-PB"]
[]
[]
[]
[]
["","","","","","EKHWCB500PBA"]
["Montáž","","","","","Podlaha"]
["Opláštenie","Farba","","","","Biela (RAL9016) / Tmavošedá (RAL7011)"]
["","Materiál","","","","Nárazu odolný polypropylén"]
["Vonkajšie rozmery","Jednotka","Výška","Nádrž","mm","1,660"]
["","","","Šírka","mm","790"]
["","","","Hĺbka","mm","790"]
["Hmotnosť","Jednotka","","Prázdna","kg","86"]
["","","","Plná","kg","586"]
["Zásobník","Objem vody","","","l","477"]
["","Materiál","","","","Polypropylén"]
["","Maximálna teplota vody","","","°C","85"]
["","Trieda energetickej účinnosti","","","","B"]
["Výmenník tepla","Teplá úžitková voda","","Množstvo","","1"]
["","","","Rúrkový materiál","","Nerezová oceľ (DIN 1.4404)"]
["","","","Objem vnútorného výmenníka","l","25.8"]
["","","","Prevádzkový tlak","tyč","6"]
["","","","Priemerný špecifický tepelný výkon","W/K","2,580"]
["","Náplň","","Množstvo","","1"]
["","","","Rúrkový materiál","","Nerezová oceľ (DIN 1.4404)"]
["","","","Objem vnútorného výmenníka","l","9"]
["","","","Prevádzkový tlak","tyč","3"]
["","","","Priemerný špecifický tepelný výkon","W/K","1,030"]
["","Pomocné solárne vyhrievanie","","Množstvo","","1"]
["","","","Rúrkový materiál","","Nerezová oceľ (DIN 1.4404)"]
["","","","Objem vnútorného výmenníka","l","4"]
["","","","Prevádzkový tlak","tyč","3"]
["","","","Priemerný špecifický tepelný výkon","W/K","350"]
["Poznámky","","","","","(1) - Tepelná strata podľa normy EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","(5) - Pre odbočkový objem 140 l -> 5820 Wh (kúpeľ) / 8 kW tepelné čerpadlo"]
["","","","","","(6) - Pre odbočkový objem 90 l -> 3660 Wh (kúpeľ) / 8 kW tepelné čerpadlo"]
["","","","","","(7) - Pre odbočkový objem 140 l -> 5820 Wh (kúpeľ) / 16kW tepelné čerpadlo"]
["","","","","","(8) - Pre odbočkový objem 90 l -> 3660 Wh (kúpeľ) / 16kW tepelné čerpadlo"]