{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":10,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWS-D3V3"]
[]
[]
[]
[]
["","","","","","EKHWS150D3V3","EKHWS180D3V3","EKHWS200D3V3","EKHWS250D3V3","EKHWS300D3V3"]
["Opláštenie","Farba","","","","Neutrálna biela","Neutrálna biela","Neutrálna biela","Neutrálna biela","Neutrálna biela"]
["","Materiál","","","","Oceľ s epoxidovým náterom, Epoxydom potiahnutá jemná oceľ","Oceľ s epoxidovým náterom, Epoxydom potiahnutá jemná oceľ","Oceľ s epoxidovým náterom, Epoxydom potiahnutá jemná oceľ","Oceľ s epoxidovým náterom, Epoxydom potiahnutá jemná oceľ","Oceľ s epoxidovým náterom, Epoxydom potiahnutá jemná oceľ"]
["Vonkajšie rozmery","Jednotka","Výška","Nádrž","mm","1,000","1,164","1,264","1,535","1,745"]
["","","","Priemer","mm","595","595","595","595","595"]
["Hmotnosť","Jednotka","","Prázdna","kg","45","50","53","58","63"]
["","","","Plná","kg","190","224","245","300","355"]
["Zásobník","Objem vody","","","l","145","174","192","242","292"]
["","Materiál","","","","Nerezová oceľ (EN 1,4521)","Nerezová oceľ (EN 1,4521)","Nerezová oceľ (EN 1,4521)","Nerezová oceľ (EN 1,4521)","Nerezová oceľ (EN 1,4521)"]
["","Maximálna teplota vody","","","°C","75","75","75","75","75"]
["","Trieda energetickej účinnosti","","","","B","B","B","B","B"]
["Výmenník tepla","Teplá úžitková voda","","Množstvo","","1","1","1","1","1"]
["","","","Rúrkový materiál","","Nerezová oceľ (EN 1.4521)","Nerezová oceľ (EN 1.4521)","Nerezová oceľ (EN 1.4521)","Nerezová oceľ (EN 1.4521)","Nerezová oceľ (EN 1.4521)"]
["","","","Objem vnútorného výmenníka","l","4.9","6.5","8.2","8.2","8.2"]
["","","","Prevádzkový tlak","tyč","10","10","10","10","10"]
["Prídavný ohrievač","Výkon","","","kW","3","3","3","3","3"]
["Poznámky","","","","","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897"]