{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKRTR"]
[]
[]
[]
[]
["","","","","EKRTR1"]
["Regulačná funkcia","","","","Pásmo proporcionality"]
["Vonkajšie rozmery","Prijímač","Výška","mm","170"]
["","","Hĺbka","mm","28"]
["","","Šírka","mm","50"]
["","Termostat","Hĺbka","mm","34"]
["","","Šírka","mm","125"]
["","","Výška","mm","87"]
["Rozsah nastavení teploty","Vykurovanie","Max.","°C","37"]
["","","Min.","°C","4"]
["","Chladenie","Max.","°C","37"]
["","","Min.","°C","4"]
["Hodiny","","","","Áno"]
["Hmotnosť","Prijímač","","g","125"]
["","Termostat","","g","210"]
["Teplota vonkajšieho prostredia","Uskladnenie","Max.","°F","140"]
["","","Min.","°C","-20"]
["","","Max.","°C","60"]
["","","Min.","°F","-4"]
["","Prevádzka","Min.","°C","0"]
["","","Max.","°F","122"]
["","","Min.","°F","32"]
["","","Max.","°C","50"]
["Maximálny menovitý spínací prúd (pri 230 VAC)","A","","","4.0 (1)"]
["Maximálna vzdialenosť k prijímaču","Vonkajší","","m","približne 100m"]
["","Vnútorný","","m","približne 30m"]
["Pripojenie","Termostat","","","Bezdrôtové"]
["","Prijímač","","","Káblové"]
["Power supply","Fáza","","","1~"]
["","Frekvencia","","Hz","50"]
["","Prijímač","Napätie","V","230"]
["","Termostat","Napätie","V","Napájané batériami 3x AA-LRG (alkalické)"]
["Poznámky","","","","(1) - 230 V AC"]