{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBH-E6V / ERRA-EV37"]
[]
[]
[]
[]
["","","","","","ELBH12EF6V / ERRA08EAV37","ELBH12EF6V / ERRA10EAV37","ELBH12EF6V / ERRA12EAV37"]
["Vykurovací výkon","Min.","","","kW","3.45 (1)","3.45 (1)","3.45 (1)"]
["","Men.","","","kW","6.17 (2)","6.17 (2)","6.17 (2)"]
["","Max.","","","kW","7.95 (1)","9.25 (1)","9.97 (1)"]
["Vstup napájania","Kúrenie","","Min.","kW","0.72 (5)","0.72 (5)","0.72 (5)"]
["","","","Men.","kW","1.25 (2)","1.25 (2)","1.25 (2)"]
["","","","Max.","kW","1.69 (5)","2.04 (5)","2.28 (5)"]
["COP","","","","","4.92 (2)","4.92 (2)","4.92 (2)"]
["Vykur. priestoru","Priemerné podnebie – výstup vody 55°C","Všeobecné","SCOP","","3.34","3.34","3.44"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A++","A++","A++"]
["","Priemerné podnebie – výstup vody 35°C","Všeobecné","SCOP","","4.69","4.71","4.71"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A+++","A+++","A+++"]
["Rozsah energetickej účinnosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Poznámky","","","","","(1) - Výkon podľa normy EN14511 a platný pre rozsah ohrievanej vody dT = 3~8°C pri Ta 7°C","(1) - Výkon podľa normy EN14511 a platný pre rozsah ohrievanej vody dT = 3~8°C pri Ta 7°C","(1) - Výkon podľa normy EN14511 a platný pre rozsah ohrievanej vody dT = 3~8°C pri Ta 7°C"]
["","","","","","(2) - Podmienka: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Podmienka: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Podmienka: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Chladenie: EW 12℃; LW 7℃; podmienky prostredia: 35° CDB","(3) - Chladenie: EW 12℃; LW 7℃; podmienky prostredia: 35° CDB","(3) - Chladenie: EW 12℃; LW 7℃; podmienky prostredia: 35° CDB"]
["","","","","","(4) - Chladenie: EW 23℃; LW 18℃; podmienky prostredia: 35° CDB","(4) - Chladenie: EW 23℃; LW 18℃; podmienky prostredia: 35° CDB","(4) - Chladenie: EW 23℃; LW 18℃; podmienky prostredia: 35° CDB"]
["","","","","","(5) - Príkon je celkový príkon vnútornej aj vonkajšej jednotky vrátane obehového čerpadla; podľa normy EN14511","(5) - Príkon je celkový príkon vnútornej aj vonkajšej jednotky vrátane obehového čerpadla; podľa normy EN14511","(5) - Príkon je celkový príkon vnútornej aj vonkajšej jednotky vrátane obehového čerpadla; podľa normy EN14511"]
["","","","","","(6) - Test pri Ta DB/WB 7°C/6°C, podľa EN 16147.","(6) - Test pri Ta DB/WB 7°C/6°C, podľa EN 16147.","(6) - Test pri Ta DB/WB 7°C/6°C, podľa EN 16147."]
["","","","","","(7) - DB/WB 7°C/6°C – LWC 35°C (dT=5°C) s čerpadlom na max. rýchlosť","(7) - DB/WB 7°C/6°C – LWC 35°C (dT=5°C) s čerpadlom na max. rýchlosť","(7) - DB/WB 7°C/6°C – LWC 35°C (dT=5°C) s čerpadlom na max. rýchlosť"]