{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBX-E9W / ERRA-EW17"]
[]
[]
[]
[]
["","","","","","ELBX12EF9W / ERRA08EAW17","ELBX12EF9W / ERRA10EAW17","ELBX12EF9W / ERRA12EAW17"]
["Vykurovací výkon","Min.","","","kW","3.45 (1)","3.45 (1)","3.45 (1)"]
["","Men.","","","kW","6.17 (2)","6.17 (2)","6.17 (2)"]
["","Max.","","","kW","7.95 (1)","9.25 (1)","9.97 (1)"]
["Chladiaci výkon","Men.","","","kW","6.81 (3), 6.47 (4)","7.97 (3), 6.47 (4)","8.62 (3), 6.47 (4)"]
["Vstup napájania","Kúrenie","","Min.","kW","0.70 (5)","0.70 (5)","0.70 (5)"]
["","","","Men.","kW","1.21 (2)","1.21 (2)","1.21 (2)"]
["","","","Max.","kW","1.63 (5)","1.98 (5)","2.21 (5)"]
["","Chladenie","","Men.","kW","2.08 (3), 1.13 (4)","2.57 (3), 1.13 (4)","2.86 (3), 1.13 (4)"]
["COP","","","","","5.10 (2)","5.10 (2)","5.10 (2)"]
["EER","","","","","3.28 (3), 5.75 (4)","5.75 (4)","3.01 (3), 5.75 (4)"]
["Vykur. priestoru","Priemerné podnebie – výstup vody 55°C","Všeobecné","SCOP","","3.58","3.58","3.58"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A++","A++","A++"]
["","Priemerné podnebie – výstup vody 35°C","Všeobecné","SCOP","","4.95","4.98","4.98"]
["","","","Trieda sezónnej účinnosti vykurovania priestoru","","A+++","A+++","A+++"]
["Rozsah energetickej účinnosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Poznámky","","","","","(1) - Výkon podľa normy EN14511 a platný pre rozsah ohrievanej vody dT = 3~8°C pri Ta 7°C","(1) - Výkon podľa normy EN14511 a platný pre rozsah ohrievanej vody dT = 3~8°C pri Ta 7°C","(1) - Výkon podľa normy EN14511 a platný pre rozsah ohrievanej vody dT = 3~8°C pri Ta 7°C"]
["","","","","","(2) - Podmienka: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Podmienka: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Podmienka: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Chladenie: EW 12℃; LW 7℃; podmienky prostredia: 35° CDB","(3) - Chladenie: EW 12℃; LW 7℃; podmienky prostredia: 35° CDB","(3) - Chladenie: EW 12℃; LW 7℃; podmienky prostredia: 35° CDB"]
["","","","","","(4) - Chladenie: EW 23℃; LW 18℃; podmienky prostredia: 35° CDB","(4) - Chladenie: EW 23℃; LW 18℃; podmienky prostredia: 35° CDB","(4) - Chladenie: EW 23℃; LW 18℃; podmienky prostredia: 35° CDB"]
["","","","","","(5) - Príkon je celkový príkon vnútornej aj vonkajšej jednotky vrátane obehového čerpadla; podľa normy EN14511","(5) - Príkon je celkový príkon vnútornej aj vonkajšej jednotky vrátane obehového čerpadla; podľa normy EN14511","(5) - Príkon je celkový príkon vnútornej aj vonkajšej jednotky vrátane obehového čerpadla; podľa normy EN14511"]
["","","","","","(6) - DB/WB 7°C/6°C – LWC 35°C (dT=5°C) s čerpadlom na max. rýchlosť","(6) - DB/WB 7°C/6°C – LWC 35°C (dT=5°C) s čerpadlom na max. rýchlosť","(6) - DB/WB 7°C/6°C – LWC 35°C (dT=5°C) s čerpadlom na max. rýchlosť"]