{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSX-E"]
[]
[]
[]
[]
["","","","","","ELSX12P30EG","ELSX12P50EG","ELSX12P30EF (Archived)","ELSX12P50EF (Archived)"]
["Opláštenie","Farba","","","","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)"]
["","Materiál","","","","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén","Nárazu odolný polypropylén"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","1891","1910","1893","1910"]
["","","","Šírka","mm","594","792","594","792"]
["","","","Hĺbka","mm","680","817","680","817"]
["Hmotnosť","Jednotka","","","kg","91.0","112","76.0","91.0"]
["PED","Kategória","","","","Kategória II","Kategória II","Kategória II","Kategória II"]
["Chladivo","Typ","","","","R-32","R-32","R-32","R-32"]
["Úroveň akustického výkonu","Men.","","","dBA","44.7","44.7","44.7","44.7"]
["Hladina akustického tlaku","Men.","","","dBA","36.8","36.8","36.8","36.8"]
["Prevádzkový rozsah","Kúrenie","Strana vody","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Max.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Chladenie","Okolitá teplota","Min.","°CDB","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Strana vody","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Max.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Napájanie","Fáza","","","","1~","1~","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50","50","50"]
["","Napätie","","","V","230","230","230","230"]
["Poznámky","","","","","(1) - V závislosti od prevádzkového režimu sa prevádzková oblasť rozšíri na nižšie prietoky – pozrite si krivku ESP.","(1) - V závislosti od prevádzkového režimu sa prevádzková oblasť rozšíri na nižšie prietoky – pozrite si krivku ESP.","(1) - V závislosti od prevádzkového režimu sa prevádzková oblasť rozšíri na nižšie prietoky – pozrite si krivku ESP.","(1) - V závislosti od prevádzkového režimu sa prevádzková oblasť rozšíri na nižšie prietoky – pozrite si krivku ESP."]
["","","","","","(2) - Tepelná strata podľa normy EN12897","(2) - Tepelná strata podľa normy EN12897","(2) - Tepelná strata podľa normy EN12897","(2) - Tepelná strata podľa normy EN12897"]
["","","","","","(3) - Viac podrobností nájdete na nákrese prevádzkového rozsahu","(3) - Viac podrobností nájdete na nákrese prevádzkového rozsahu","(3) - Viac podrobností nájdete na nákrese prevádzkového rozsahu","(3) - Viac podrobností nájdete na nákrese prevádzkového rozsahu"]