{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","740"]
["","","","Šírka","mm","884"]
["","","","Hĺbka","mm","388"]
["Hmotnosť","Jednotka","","","kg","58.5"]
["Prevádz. rozsah","Chladenie","","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["Prevádzkový rozsah","Teplá úžitková voda","","Min.","°CDB","-25"]
["Prevádz. rozsah","Teplá pitná voda","","Max.","°CDB","35"]
["Úroveň akustického výkonu","Kúrenie","","Men.","dBA","58 (1)"]
["","Chladenie","","Men.","dBA","61 (1)"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","44 (1)"]
["","Chladenie","","Men.","dBA","48 (1)"]
["Chladivo","Typ","","","","R-32"]
["","GWP","","","","675.0"]
["","Náplň","","","tCO2Eq","1.01"]
["","Náplň","","","kg","1.50"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6"]
["","Plyn","","OD","mm","15.9"]
["Pripojenia potrubí","Vypúšťanie","","OD","mm","18"]
["","Úroveň hladiny","IU - OU","Max.","m","20.0"]
["Pripojenia potrubia","Tepelná izolácia","","","","Potrubí kvapaliny aj plynu"]
["Napájanie","Názov","","","","V3"]
["","Fáza","","","","1N~"]
["Zdroj napájania","Frekvencia","","","Hz","50"]
["","Napätie","","","V","230"]
["Prúd","Odporúčané poistky","","","A","20"]
["Poznámky","","","","","(1) - Chladenie Ta 35°C - LWE 18°C (DT = 5°C); ohrievanie Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]