{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AV1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAV1","ERSQ014AAV1","ERSQ016AAV1"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","","53"]
["Štandardné príslušenstvo","Návod na montáž","","","","","1"]
["Chladivo","GWP","","","","","2,087.5"]
["","Charge","","","kg","","4.5"]
["","Typ","","","","","R-410A"]
["Prevádzkový rozsah","Kúrenie","","Max.","°CWB","","20"]
["","","","Min.","°CWB","","-20"]
["","Teplá úžitková voda","","Min.","°CDB","","-20"]
["","","","Max.","°CDB","","35"]
["Pripojenia potrubí","Tepelná izolácia","","","","","Potrubí kvapaliny aj plynu"]
["","Kvapalina","","OD","mm","","9.52"]
["","Plyn","","OD","mm","","15.9"]
["","Vypúšťanie","","OD","mm","","26x3"]
["","Úroveň hladiny","IU - OU","Max.","m","","30"]
["Úroveň akustického výkonu","Kúrenie","","Men.","dBA","","69"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","","900"]
["","","","Hĺbka","mm","","320"]
["","","","Výška","mm","","1,345"]
["Hmotnosť","Jednotka","","","kg","","120"]
["Power supply","Fáza","","","","","1~"]
["","Názov","","","","","V1"]
["","Frekvencia","","","Hz","","50"]
["","Napätie","","","V","","220-440"]
["Prúd","Odporúčané poistky","","","A","","25"]
["Poznámky","","","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","(2) - Zmax: V súlade s normou EN/IEC 61000-3-11, môže byť potrebná konzultácia s operátorom rozvodnej siete, aby sa zaistilo, že bude zariadenie pripojené iba k zdroju s hodnotou Zsys (impedancia systému) ≤ Zmax."]
["","","","","","","(3) - EN/IEC 61000-3-11: Európska/medzinárodná technická norma určujúca limity pre zmeny napätia, napäťové výkyvy a kmitanie vo verejných systémoch s dodávkou nízkeho napätia pre zariadenia s menovitým príkonom ≤ 75A"]
["","","","","","","(4) - Min. hodnota Ssc (= Skratový výkon): Zariadenie vyhovujúce norme EN/IEC 61000-3-12: Európska/medzinárodná technická norma určujúca limity pre harmonické prúdy generované zariadeniami pripojenými k verejným systémom s nízkym napätím s príkonom > 16 A a ≤ 75 A na fázu"]
["","","","","","","(5) - Obsahuje fluórované skleníkové plyny"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","1345","","1345"]
["","","","Šírka","mm","900","","900"]
["","","","Hĺbka","mm","320","","320"]
["Hmotnosť","Jednotka","","","kg","120","","120"]
["Prevádzkový rozsah","Kúrenie","","Min.","°CWB","-20","","-20"]
["","","","Max.","°CWB","20","","20"]
["","Teplá úžitková voda","","Min.","°CDB","-20","","-20"]
["Prevádz. rozsah","Teplá pitná voda","","Max.","°CDB","35","","35"]
["Úroveň akustického výkonu","Kúrenie","","Men.","dBA","68","","71"]
["Hladina akustického tlaku","Kúrenie","","Men.","dBA","52","","55"]
["Chladivo","Typ","","","","R-410A","","R-410A"]
["","GWP","","","","2087.5","","2087.5"]
["","Náplň","","","tCO2Eq","9.4","","9.4"]
["","Náplň","","","kg","4.5","","4.5"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52","","9.52"]
["","Plyn","","OD","mm","15.9","","15.9"]
["Pripojenia potrubí","Vypúšťanie","","OD","mm","26x3","","26x3"]
["","Úroveň hladiny","IU - OU","Max.","m","30","","30"]
["Pripojenia potrubia","Tepelná izolácia","","","","Potrubí kvapaliny aj plynu","","Potrubí kvapaliny aj plynu"]
["Štandardné príslušenstvo","Installation manual","","","","1","","1"]
["Napájanie","Názov","","","","V1","","V1"]
["","Fáza","","","","1~","","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","","50"]
["","Napätie","","","V","220-440","","220-440"]
["Prúd","Odporúčané poistky","","","A","25","","25"]