{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH16E"]
[]
[]
[]
[]
["","","","","","ETSH16P50EF","ETSH16P30EF"]
["Opláštenie","Farba","","","","Biela (RAL9016)/Čierna (RAL9017)","Biela (RAL9016)/Čierna (RAL9017)"]
["","Materiál","","","","Nárazu odolný polypropylén","Nárazu odolný polypropylén"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","1,910","1,892"]
["","","","Šírka","mm","792","594"]
["","","","Hĺbka","mm","816","644"]
["Hmotnosť","Jednotka","","","kg","98","75"]
["Akustický výkon","Nom.","","","dBA","45.6","45.6"]
["Hladina akustického tlaku","Men.","","","dBA","32.8","32.8"]
["Prevádzkový rozsah","Kúrenie","Strana vody","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["","Chladenie","Okolitá teplota","Min.","°CDB","0 (2)","0 (2)"]
["","","Strana vody","Min.","°C","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)"]
["Power supply","Fáza","","","","1~","1~"]
["","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","230","230"]
["Poznámky","","","","","(1) - Tepelná strata podľa normy EN12897","(1) - Tepelná strata podľa normy EN12897"]
["","","","","","(2) - Pozrite si výkresy prevádzkových obmedzení","(2) - Pozrite si výkresy prevádzkových obmedzení"]