{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Opláštenie","Farba","","","","Biela","Biela"]
["","Materiál","","","","Živica","Živica"]
["Vonkajšie rozmery","Jednotka","","Výška","mm","290","340"]
["","","","Šírka","mm","1050","1200"]
["","","","Hĺbka","mm","269","262"]
["Hmotnosť","Jednotka","","","kg","14","18"]
["Ventilátor","Prietok vzduchu","Chladenie","Vysoké","m³/min","16.2","23"]
["","","","Stredný","m³/min","13.4","21.1"]
["","","","Nízka","m³/min","12.1","18.7"]
["","","Kúrenie","Vysoké","m³/min","16.9","23"]
["","","Vykurovanie","Stredný","m³/min","14.2","20.9"]
["","","Kúrenie","Nízka","m³/min","12.7","18.7"]
["Akustický výkon","Chladenie","","","dBA","61","65"]
["","Vykurovanie","","","dBA","61","65"]
["Hladina akustického tlaku","Chladenie","","Vysoké","dBA","45","49"]
["","","","Stredný","dBA","42","45"]
["","","","Nízka","dBA","40","41"]
["","Kúrenie","","Vysoké","dBA","45","49"]
["","Vykurovanie","","Stredný","dBA","42","45"]
["","Kúrenie","","Nízka","dBA","40","41"]
["Pripojenia potrubia","Kvapalina","","OD","mm","9.52","9.52"]
["","Plyn","","OD","mm","15.9","15.9"]
["","Odvod kondenzátu","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Napájanie","Fáza","","","","1~","1~"]
["Zdroj napájania","Frekvencia","","","Hz","50","50"]
["","Napätie","","","V","220-240","220-240"]
["Štandardné príslušenstvo","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Poznámky","","","","","(1) - Nom. chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Štandardné príslušenstvo","Screw cover","","","","","3"]