{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B (Archived)"]
["Outdoor unit","","","","AZAS71M2V1B"]
["Chladiaci výkon","Men.","","kW","6.80"]
["Vykurovací výkon","Men.","","kW","7.50"]
["Chladenie","Trieda energetickej účinnosti","","","A"]
["","Výkon","P návrh","kW","6.80"]
["","SEER","","","5.57"]
["","Ročná spotreba energie","","kWh/rok","427"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","A"]
["","Výkon","P návrh","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Ročná spotreba energie","","kWh/rok","1654"]
["Poznámky","","","","(1) - Chladenie: T2: vnút. tepl. 26,6°CDB, 19,4°CWB, vonk. tepl. 48°CDB [Btu/h/W]"]
["","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]