{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Hladina akustického tlaku","Kúrenie","","Vysoké","dBA","37.0","37.0","31.0","31.0"]
["","","","Stredný","dBA","34.0","34.0","28.0","28.0"]
["","","","Nízka","dBA","29.0","29.0","25.0","25.0"]
["","Chladenie","","Stredný","dBA","32.0","32.0","28.0","28.0"]
["","","","Nízka","dBA","29.0","29.0","25.0","25.0"]
["","","","Vysoké","dBA","35.0","35.0","30.0","30.0"]
["Štandardné príslušenstvo","Návod na prevádzku","","","","1","1","1","1"]
["","Návod na montáž","","","","1","1","1","1"]
["","Vypúšťacia hadica","","","","1","1","1","1"]
["","Kovová svorka pre odvodovú hadicu","","","","1","1","1","1"]
["","Podložka pre držiak ramena","","","","8","8","8","8"]
["","Skrutky","","","","40","40","40","40"]
["","Izolácia príslušenstva","","","","2","2","2","2"]
["","Tesniace podložky","","","","5","5","5","5"]
["","Svorky","","","","4","4","4","4"]
["Riadiace systémy","Káblový diaľkový ovládač","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infra. diaľkové ovládanie","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Pripojenia potrubia","Kvapalina","","OD","mm","6.35","6.35","6.35","9.52"]
["","Plyn","","OD","mm","9.52","12.70","12.70","15.90"]
["","Vypúšťanie","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Akustický výkon","Chladenie","","","dBA","60","60","56","56"]
["Vonkajšie rozmery","Jednotka","","Šírka","mm","700","700","1,000","1,000"]
["","","","Hĺbka","mm","800","800","800","800"]
["","","","Výška","mm","245","245","245","245"]
["Opláštenie","Materiál","","","","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech","Pozinkovaný oceľový plech"]
["","Farba","","","","Nenatretý (pozinkovaný)","Nenatretý (pozinkovaný)","Nenatretý (pozinkovaný)","Nenatretý (pozinkovaný)"]
["Hmotnosť","Jednotka","","","kg","28.0","28.0","35.0","35.0"]
["Ventilátor","Atmosférický tlak vonkajšieho prostredia","","Vysoký","Pa","150","150","150","150"]
["","","","Nom. ot.","Pa","30","30","30","30"]
["","Prietok vzduchu","Kúrenie","Vysoké","m³/min","15.0","15.0","18.0","18.0"]
["","","","Nízka","m³/min","10.5","10.5","12.5","12.5"]
["","","","Stredný","m³/min","12.5","12.5","15.0","15.0"]
["","","Chladenie","Nízka","m³/min","10.5","10.5","12.5","12.5"]
["","","","Stredný","m³/min","12.5","12.5","15.0","15.0"]
["","","","Vysoké","m³/min","15.0","15.0","18.0","18.0"]
["Výška odsávania","mm","","","","625","625","625","625"]
["Power supply","Fáza","","","","1~","1~","1~","1~"]
["","Frekvencia","","","Hz","50/60","50/60","50/60","50/60"]
["","Napätie","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Poznámky","","","","","(1) - Hladina zvuku je absolútna hodnota, ktorá uvádza výkon, ktorý generuje zdroj zvuku.","(1) - Hladina zvuku je absolútna hodnota, ktorá uvádza výkon, ktorý generuje zdroj zvuku.","(1) - Hladina zvuku je absolútna hodnota, ktorá uvádza výkon, ktorý generuje zdroj zvuku.","(1) - Hladina zvuku je absolútna hodnota, ktorá uvádza výkon, ktorý generuje zdroj zvuku."]
["","","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch"]