{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Chladiaci výkon","Men.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Vykurovací výkon","Men.","","kW","","","","","","","","","","","","","","","","7.50","","","15.50"]
["Nominálna účinnosť","EER","","","","","","","","","","","","","","","","3.30","3.30","3.39","3.30","3.39","2.50"]
["","COP","","","","","","","","","","","","","","","","","","3.97","","","3.61"]
["","Ročná spotreba energie","","kWh","","","","","","","","","","","","","","","","1,003"]
["","Smernica o energetickom označovaní","Chladenie","","","","","","","","","","","","","","","","","A"]
["","","Vykurovanie","","","","","","","","","","","","","","","","","A"]
["Chladenie priestoru","Trieda energetickej účinnosti","","","","","","","","","","","","","","","","A","A","A++","A","A++"]
["","Výkon","P návrh","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10","6.72","5.10","6.80","6.44"]
["","Ročná spotreba energie","","kWh/a","","","","","","","","","","","","","","467","467","355","467","350","1,249"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","","","","","","","","","","","","","A","A","A+","A","A+"]
["","Výkon","P návrh","kW","","","","","","","","","","","","","","6.00","6.00","6.33","6.00","6.33","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80","4.20","3.80","4.20","4.27"]
["","Ročná spotreba energie","","kWh/a","","","","","","","","","","","","","","2,211","2,211","2,110","2,211","2,110","3,795"]
["Poznámky","","","","","","","","","","","","","","","","","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","","","","","","","","","","","","","","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["Rozsah energetickej účinnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Poznámky","","","","","","","","","","","","","","","","","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese","","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","","","","","","","","","","","","","(4) - Elektrické údaje nájdete v samostatných nákresoch","(4) - Elektrické údaje nájdete v samostatných nákresoch","","","(4) - Elektrické údaje nájdete v samostatných nákresoch"]