{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":13,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Chladiaci výkon","Men.","","kW","","","6.80 (1)","","","","","","13.4 (1)"]
["Chladenie priestoru","SEER","","","","","6.91","6.91","","","","","6.75"]
["","ηs, c","","%","","","","","","","","","266.9"]
["","Ročná spotreba energie","","kWh/a","","","345","345","","","","","1,191"]
["","Výkon","P návrh","kW","","","6.80","6.80","","","","","13.4"]
["","Trieda energetickej účinnosti","","","","","A++","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","","","7.60","7.60","","","","","11.8"]
["","SCOP/A","","","","","4.54","4.54","","","","","4.38"]
["","Trieda energetickej účinnosti","","","","","A+","A+"]
["","Ročná spotreba energie","","kWh/a","","","2,344","2,344","","","","","3,766"]
["","ηs, h","","%","","","","","","","","","172.1"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","","","830"]
["","EER","","","","","4.09 (3)","","","","","","3.18 (3)"]
["","COP","","","","","4.80 (3)","","","","","","4.12 (3)"]
["","Smernica o energetickom označovaní","Chladenie","","","","A"]
["","","Vykurovanie","","","","A"]
["Vykurovací výkon","Men.","","kW","","","7.50 (2)","","","","","","15.5 (2)"]
["Poznámky","","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m","","","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m"]
["","","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m","","","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]
["","","","","","","(3) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","","","","","","(3) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]
["Rozsah energetickej účinnosti","","","","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Vonkajšia jednotka","","","","","","","","","RZQG100L8Y1","","RZQG125L8Y1"]
["Chladenie","Trieda energetickej účinnosti","","","","","","","","A","","A"]
["","Výkon","P návrh","kW","","","","","","9.50","","12.0"]
["","SEER","","","","","","","","5.10","","5.10"]
["","Ročná spotreba energie","","kWh/a","","","","","","652","","824"]
["Vykurovanie (stredné klim. pásmo)","Trieda energetickej účinnosti","","","","","","","","A","","A"]
["","Výkon","P návrh","kW","","","","","","11.30","","12.71"]
["","SCOP/A","","","","","","","","3.80","","3.80"]
["","Pdh Vykurovací výkon pri -10°","","kW","","","","","","9.66","","11.4"]
["","Ročná spotreba energie","","kWh/a","","","","","","4164","","4683"]