{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQSG100L8Y1B","FCAHG140GVEB / RZQSG140L7Y1B"]
["Chladiaci výkon","Men.","","kW","9.50 (1)","13.4 (1)"]
["Chladenie priestoru","SEER","","","6.70"]
["","Ročná spotreba energie","","kWh/a","497"]
["","Výkon","P návrh","kW","9.50"]
["","Trieda energetickej účinnosti","","","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","8.03"]
["","SCOP/A","","","4.30"]
["","Trieda energetickej účinnosti","","","A+"]
["","Ročná spotreba energie","","kWh/a","2,615"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","1,285"]
["","EER","","","3.70 (3)","3.11 (3)"]
["","COP","","","4.30 (3)","3.61 (3)"]
["","Smernica o energetickom označovaní","Chladenie","","A"]
["","","Vykurovanie","","A"]
["Vykurovací výkon","Men.","","kW","10.8 (2)","15.5 (2)"]
["Poznámky","","","","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m","(1) - Chladenie: vnútorná teplota 27°CDB, 19°CWB; vonkajšej teplote 35 °CDB; ekvivalentná dĺžka potrubia: 7,5m; výškový rozdiel: 0m"]
["","","","","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m","(2) - Kúrenie: vnútorná teplota 20°CDB; vonkajšej teplote 7°CDB, 6°CWB; príslušnej dĺžky potrubia chladiva: 7,5 m; výškový rozdiel: 0m"]
["","","","","(3) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ","(3) - EER/COP podľa Eurovent 2012 na použitie len mimo EÚ"]