{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-H / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG71HVEB / FCAHG71HVEB / RZQG100L8Y1B","FCAHG71HVEB / FCAHG71HVEB / RZQG125L8Y1B","FCAHG140HVEB / RZQG100L8Y1B","FCAHG140HVEB / RZQG125L8Y1B","FCAHG125HVEB / RZQG125L8Y1B","FCAHG100HVEB / RZQG100L8Y1B","FCAHG71HVEB / RZQG71L8Y1B","FCAHG100HVEB / RZQG71L8Y1B","FCAHG140HVEB / RZQG140L7Y1B"]
["Rozsah energetickej účinnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Chladiaci výkon","Men.","","kW","","","","","","","6.80","6.80","13.40"]
["Chladenie priestoru","SEER","","","","","","","","","6.91","6.91","6.75"]
["","Ročná spotreba energie","","kWh/a","","","","","","","345","345","1,191"]
["","Výkon","P návrh","kW","","","","","","","6.80","6.80","13.40"]
["","Trieda energetickej účinnosti","","","","","","","","","A++","A++"]
["Vykurovanie (stredné klim. pásmo)","Výkon","P návrh","kW","","","","","","","7.60","7.60","11.78"]
["","SCOP/A","","","","","","","","","4.54","4.54","4.38"]
["","Trieda energetickej účinnosti","","","","","","","","","A+","A+"]
["","Ročná spotreba energie","","kWh/a","","","","","","","2,344","2,344","3,766"]
["Nominálna účinnosť","Ročná spotreba energie","","kWh","","","","","","","831"]
["","EER","","","","","","","","","4.09","4.09","3.18"]
["","COP","","","","","","","","","4.80","","4.12"]
["","Smernica o energetickom označovaní","Chladenie","","","","","","","","A"]
["","","Vykurovanie","","","","","","","","A"]
["Vykurovací výkon","Men.","","kW","","","","","","","7.50","","15.50"]
["Poznámky","","","","","","","","","","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;","(1) - Prevádzkový rozsah nájdete v samostatnom výkrese","(1) - Nominálny chladiaci výkon závisí od: vnútornej teploty: 27°CDB, 19°CWB, vonkajšej teploty: 35 °CDB, príslušnej dĺžky potrubia chladiva: 5 m, prevýšenia: 0 m;"]
["","","","","","","","","","","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m.","(2) - Elektrické údaje nájdete v samostatných nákresoch","(2) - Nominálny výkon vyhrievania závisí od: vnútornej teploty: 20 °CDB, vonkajšej teploty: 7°CDB, 6°CWB, príslušnej dĺžky potrubia chladiva: 5m, úrovňového rozdielu: 0m."]
["","","","","","","","","","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese","","(3) - Prevádzkový rozsah nájdete v samostatnom výkrese"]
["","","","","","","","","","","(4) - Elektrické údaje nájdete v samostatných nákresoch","","(4) - Elektrické údaje nájdete v samostatných nákresoch"]
["Chladenie priestoru","ηs, c","","%","","","","","","","","","266.88"]
["Vykurovanie (stredné klim. pásmo)","ηs, h","","%","","","","","","","","","172.10"]